{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["ETS","Dry Block","Baths","Pressure Calibrator","Cal EQ - Rental","Version Control"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":20,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ETS","index":0,"n_rows":43,"n_cols":10,"rows_kept":43,"cut":false,"hidden":false,"merged":[[41,1,41,9],[34,1,34,9],[39,1,39,9],[0,8,1,9],[9,1,9,9],[18,1,18,9],[25,1,25,9],[29,1,29,9],[10,1,10,9],[12,1,12,9],[14,1,14,9],[16,1,16,9],[21,1,21,9]]}
[null,"Ellab Calibration Solutions",null,null,null,null,null,null,{"$error":"#VALUE!"}]
[null,"Parts List: Ellab Temperature Standard"]
[null,"Calibration Pricing Ver. 02 - June 2026"]
[null,"1 January 2026 to 31 December 2026"]
[null,null,null,null,null,"DKK/€","DKK/£","DKK/$","DKK/CHF","DKK/Japan US"]
[null,null,null,null,null,{"$f":"'Version Control'!$E$6","v":7.43},{"$f":"'Version Control'!$F$6","v":8.6},{"$f":"'Version Control'!$G$6","v":6},{"$f":"'Version Control'!$H$6","v":7.7},{"$f":"'Version Control'!$I$6","v":5.5}]
[null,"Description","Ellab Ordering\nCode","RRP DKK","Discount","RRP €","RRP £","RRP US$","RRP CHF","Japan US$"]
[null,"ELLAB TEMPERATURE STANDARD"]
[null,"ETS"]
[null,"Sensor lenght 300mm\nProbe 100 Ohm\nUSB/PoE connection.\nIncl. Accredited Calibration Certificate and Suitecase."]
[null,"ETS 10\nTemperature Range: -80°C to +250°C\nAccuracy: +/- 0.015°C./0.025°C"]
[null,"ETS10 TEMPERATURE STANDARD",20000195,52646,null,7086,6122,8774,6837,9572]
[null,"ETS 20\nTemperature Range: -50°C. to +150°C\nAccuracy: +/- 0.02°C"]
[null,"ETS20 TEMPERATURE STANDARD",20000196,42966,null,5783,4996,7161,5580,7812]
[null,"ETS 25 Standard\nTemperature Range: -196 °C to 420 °C\nAccuracy: +/- 0.025 °C"]
[null,"ETS25 TEMPERATURE STANDARD",20000197,57518,null,7741,6688,9586,7470,10458]
[null,"ETS 25 Standard Angled\nTemperature Range: -45 °C to +150 °C\nAccuracy: +/- 0.025 °C"]
[null,"ETS25 A182 ANGLED TEMPERATURE STANDARD",20000198,46161,null,6213,5368,7694,5995,8393]
[null,"ETS 25 Standard Angled\nTemp: -95 °C to +150 °C\nAccuracy: +/- 0.025 °C"]
[null,"ETS25 A213 ANGLED TEMPERATURE STANDARD",20000199,52661,null,7088,6123,8777,6839,9575]
[null,"Accessories"]
[null,"ETS Optional Display for stand-alone usage"]
[null,"ETS OPTIONAL DISPLAY",20000095,11170,null,1503,1299,1862,1451,2031]
[]
[null,"SOFTWARE"]
[null,"Software for ETS with graphical presentation of data for up to 5 individual color coded ETS systems. \nZoom function and print function as well as export facility (Excel). NOT for XP. Including license for one user/computer"]
[null,"ETS SUITE SOFTWARE WIN 7",20000118,5966,null,803,694,994,775,1085]
[]
[null,"SUITCASES"]
[null,"Suitcase for 1 pcs. ETS and accessories. \nDimensions: 45x36x10.6 cm"]
[null,"SUITCASE FOR ETS 3G",21202001,3123,null,420,363,521,406,568]
[]
[null,"CALIBRATION"]
[null,"STANDARD CALIBRATION CERTIFICATE"]
[null,"ETS 10: Accredited Calibration Certificate for ETS 10, Calibration points: -80, -50, -25, 0, +90, +150, +250°C\nETS 20: Accredited Calibration Certificate for ETS 20 Calibration points:  -50, -25, 0, +90, +150°C\nETS 25: Accredited Calibration Certificate for ETS 25 Calibration points:  -196, -50,  0, +150, +420°C "]
[null,"CALIBRATION CERTIFICATE ETS 10",20000098,11482,null,1545,1335,1914,1491,2088]
[null,"CALIBRATION CERTIFICATE ETS 20",20000096,6112,null,823,711,1019,794,1111]
[null,"CALIBRATION CERTIFICATE ETS 25",20000097,8796,null,1184,1023,1466,1142,1599]
[null,"NON-STANDARD CALIBRATION CERTIFICATE"]
[null,"NEW ITEM are available for quoting from Februrary 1st, 2026.\nMandatory start-up fee for other calibration points than already defined as standard points."]
[null,"Calibration - Start-Up Fee for Extra Check Points",9000170,996,null,134,116,166,129,181]
[null,"Extra calibration charge for other calibration points than already defined as standard points."]
[null,"Calibration - ETS - Charge for other additional calibration points",20000089,2600,null,350,302,433,338,473]

{"sheet":"Dry Block","index":1,"n_rows":84,"n_cols":10,"rows_kept":84,"cut":false,"hidden":false,"merged":[[67,1,67,9],[70,1,70,2],[82,1,82,9],[80,1,80,9],[0,8,1,9],[9,1,9,9],[22,1,22,9],[25,1,25,2],[37,1,37,9],[40,1,40,2],[49,1,49,9],[52,1,52,2]]}
[null,"Ellab Calibration Solutions",null,null,null,null,null,null,{"$error":"#VALUE!"}]
[null,"Parts List: Dry Block"]
[null,"Calibration Pricing Ver. 02 - June 2026"]
[null,"1 January 2026 to 31 December 2026"]
[null,null,null,null,null,"DKK/€","DKK/£","DKK/$","DKK/CHF","DKK/Japan US"]
[null,null,null,null,null,7.43,8.6,6,7.7,5.5]
[null,"Description","Ellab Ordering\nCode","RRP DKK","Discount","RRP €","RRP £","RRP US$","RRP CHF","Japan US$"]
[null,"DRY BLOCK - PTC-155"]
[null,"DRY BLOCK"]
[null,"Dry Block: PTC-155A temperature dryblock model without input option.\nTemperature Range: -25 to +155°C; Weight: 10.3 kg; Power Supply: 115-230 V/50-60 Hz\nExcluding Carrying Case and Insert"]
[null,"DRYBLOCK PTC-155A",20000155,90615,null,12196,10537,15103,11768,16475]
[null,"INSERT"]
[null,"Insert for PTC 155A with hole dimensions of 18 x ø2,2 mm + 1 x ø6.55 mm (ETS) incl. insulation plug"]
[null,"INSERT 18 x 2,2 FOR PTC 155A","20001155Y",10981,null,1478,1277,1830,1426,1997]
[null,"Insert for PTC 155A with hole dimensions of 16 x ø2,8 mm + 1 x ø6.55 mm (ETS) incl. insulation plug"]
[null,"INSERT 16 x 2,8 FOR PTC 155A","20001155W",9876,null,1329,1148,1646,1283,1796]
[null,"CARRYING CASE"]
[null,"Carrying Case Type CX for PTC model 155/350/425"]
[null,"CARRYING CASE FOR PTC 155/350/425",20002155,8383,null,1128,975,1397,1089,1524]
[]
[null,"DRY BLOCK - RTC-156"]
[null,"DRY BLOCKS"]
[null,"Dry Block: RTC 156A temperature dry block model without input option.\nTemperature Range: -30 to +155°C; Weight : 10.5 kg; Power Supply: 115-230 V/50-60 Hz\nExcluding Carrying Case and Insert"]
[null,"DRYBLOCK RTC-156A",20000156,111854,null,15054,13006,18642,14526,20337]
[null,"INSERT"]
[null,"Insert for RTC 156 with hole dimensions of 24 x ø2.2 mm + 1 x ø6.55 mm (ETS) incl. insulation plug\nIMPORTANT: Do not use with ø2.0 TSP high temp. sensors"]
[null,"INSERT 24 x 2,2 FOR RTC 156","20001156X",11372,null,1531,1322,1895,1477,2068]
[null,"Insert for RTC 156 with hole dimensions of 24 x ø2.8 mm + 1 x ø6.55 mm (ETS) incl. insulation plug"]
[null,"Multihole Insert 24 x 2.8mm & 1 x 6.55mm for RTC-156/157/159/PTC-12","20001156Y",11372,null,1531,1322,1895,1477,2068]
[null,"Insert for RTC 156 with hole dimensions of 20 x ø3,5 mm + 1 x ø6.55 mm (ETS) incl. insulation plug"]
[null,"Multihole Insert - 20 x 3.5mm & 1 x 6.55 mm","20001156Z",10813,null,1455,1257,1802,1404,1966]
[null,"CARRYING CASE"]
[null,"Carrying Case with Trolley type CT for PTC 155/350/660 & RTC 156/157/158/168"]
[null,"CARRYING CASE TROLLEY FOR PTC/RTC",20002156,11763,null,1583,1368,1961,1528,2139]
[]
[null,"DRY BLOCK - RTC-159"]
[null,"DRY BLOCK"]
[null,"Dry Block: RTC 159A temperature dry block model without input option. \nTemperature Range: -100 to +155°C; Weight: 15.2 kg; Power Supply: 115-230 V/50-60 Hz\nIncluding Carrying Case (16.5 kg). Excluding Insert"]
[null,"DRYBLOCK RTC-159A",20000159,221328,null,29788,25736,36888,28744,40241]
[null,"INSERT"]
[null,"Insert for RTC 159 with hole dimensions of 24 x ø2.2 mm + 1 x ø6.55 mm (ETS) incl. insulation plug"]
[null,"Multihole Insert 24 x 2.2mm & 1 x 6.55mm for RTC-156/157/159/PTC-125","20001159X",11372,null,1531,1322,1895,1477,2068]
[null,"Insert for RTC 159 with hole dimensions of 24 x ø2.8 mm + 1 x ø6.55 mm (ETS) incl. insulation plug"]
[null,"INSERT 24 x Ø2,8 FOR RTC 159","20001159Y",11371.8,null,1531,1322,1895,1477,2068]
[null,"Insert for RTC 159 with hole dimensions of 20 x ø3,5 mm + 1 x ø6.55 mm  (ETS) incl insulation plug"]
[null,"INSERT 20 x Ø3,5 FOR RTC 159","20001159Z",10930,null,1471,1271,1822,1419,1987]
[]
[null,"DRY BLOCK - RTC-168"]
[null,"DRY BLOCK"]
[null,"Dry Block: RTC 168A temperature dry block/ liquid bath. Basic Model without input.\nTemperature Range: -30°C to 165°C; Weight: 11 kg; Power Supply: 115-230 V/50-60 Hz\nExcl. Carrying Case, Liquid Bath Kit and Inserts"]
[null,"DRYBLOCK RTC-168A",20000168,127226,null,17123,14794,21204,16523,23132]
[null,"INSERT"]
[null,"Insert for RTC 168 with hole dimension of 16 x ø9,0 mm + 1 x ø6,55 (ETS) incl insulation plug"]
[null,"INSERT 16 x 9,0 FOR RTC 168","20001168W",13280,null,1787,1544,2213,1725,2415]
[null,"DIVIDER"]
[null,"Divider for RTC 168 insert allowing a total of 48 sensors ø3,2 mm (set of 16 pcs)"]
[null,"DIVIDER 3PCS 3,5mm FOR RTC 168","20001168V",7680,null,1034,893,1280,997,1396]
[null,"Divider for RTC 168 insert allowing a total of 48 sensors ø2,5 mm (set of 16 pcs)"]
[null,"DIVIDER 3PCS 2,8mm FOR RTC 168","20001168U",4544,null,612,528,757,590,826]
[null,"Divider for RTC 168 insert allowing a total of 48 sensors ø1,8 mm (set of 16 pcs)"]
[null,"DIVIDER 3PCS 2,2mm FOR RTC 168","20001168T",7680,null,1034,893,1280,997,1396]
[null,"LIQUID BATH KIT"]
[null,"Liquid Bath Kit incl. container"]
[null,"LIQUID BATH KIT","20001168KIT2",8979,null,1208,1044,1497,1166,1633]
[]
[null,"DRY BLOCK - PTC-425"]
[null,"DRY BLOCK"]
[null,"Dry Block: PTC 425A Temperature dry block model without input option.\nTemperature Range: +33 to +425°C; Weight: 8.2 kg; Power Supply: 115-230 V/50-60 Hz\nExcluding Carrying Case and Insert"]
[null,"DRYBLOCK PTC-425A",20000425,91158,null,12269,10600,15193,11839,16574]
[null,"INSERT"]
[null,"Insert for PTC 425 with hole dimensions of 18 x ø2.2 mm + 1 x ø6.55 mm (ETS) without insulation plug"]
[null,"INSERT 18 x 2,2 PTC-425","20001425V",18808,null,2531,2187,3135,2443,3420]
[null,"Insert for PTC 425 with hole dimensions of 16 x ø2.8 mm + 1 x ø6.55 mm (ETS) without insulation plug"]
[null,"INSERT 16 x 2,8 PTC-425","20001425W",11322.3,null,1524,1317,1887,1470,2059]
[null,"Insert for PTC 425 with hole dimensions of 12 x ø3.2 mm + 1 x ø6.55 mm (ETS) without insulation plug"]
[null,"INSERT 12 x 3,2 PTC-425","20001425Y",10947,null,1473,1273,1825,1422,1990]
[null,"Insert for PTC 425 with hole dimensions of 12 x ø3.5 mm + 1 x ø6.55 mm (ETS) without insulation plug"]
[null,"INSERT 12 x 3,5 PTC-425","20001425Z",10947,null,1473,1273,1825,1422,1990]
[]
[null,"ACCESSORIES"]
[null,"Logger support for RTC / PTC dryblocks including height  adjustable plate (185 x 170 mm) holding 20 loggers and 1 ETS complete with two support rods"]
[null,"LOGGER SUPPORT FOR RTC/PTC DRYBLOCKS",20004100,3369,null,453,392,562,438,613]
[null,"Logger support for RTC159 for holding 25 loggers"]
[null,"LYOPRO SUPPORT FRAME FOR RTC159",20004101,2042,null,275,237,340,265,371]

{"sheet":"Baths","index":2,"n_rows":55,"n_cols":10,"rows_kept":55,"cut":false,"hidden":false,"merged":[[44,1,44,9],[22,1,22,9],[26,1,26,9],[38,1,38,9],[41,1,41,9],[24,1,24,9],[28,1,28,9],[30,1,30,9],[0,8,1,9],[9,1,9,9],[33,1,33,9],[35,1,35,9],[11,1,11,9],[13,1,13,9],[15,1,15,9],[17,1,17,9]]}
[null,"Ellab Calibration Solutions",null,null,null,null,null,null,{"$error":"#VALUE!"}]
[null,"Parts List: Baths"]
[null,"Calibration Pricing Ver. 02 - June 2026"]
[null,"1 January 2026 to 31 December 2026"]
[null,null,null,null,null,"DKK/€","DKK/£","DKK/$","DKK/CHF","DKK/Japan US"]
[null,null,null,null,null,7.43,8.6,6,7.7,5.5]
[null,"Description","Ellab Ordering\nCode","RRP DKK","Discount","RRP €","RRP £","RRP US$","RRP CHF","Japan US$"]
[null,"LIQUID BATHS - FLOOR MODEL"]
[null,"FLOOR MODEL"]
[null,"LiquiCal SL 230V/50Hz \nTemperature Range: -45°C to +150°C; Volume: 15,9 l; Weight: 68 kg"]
[null,"LIQUICAL SL 230V/50Hz",20100141,182004,null,24496,21163,30334,23637,33092]
[null,"LiquiCal SL 115V/60Hz\nTemperature Range: -45°C to +150°C; Volume: 15,9 l; Weight: 68 kg"]
[null,"LIQUICAL SL 115V/60Hz",20100151,182004,null,24496,21163,30334,23637,33092]
[null,"LiquiCal LL 115V/60Hz\nTemperature Range: -80°C to +110°C; Volume: 15,9 l; Weight: 91 kg"]
[null,"LIQUICAL LL 115V/60Hz",20100140,274072,null,36887,31869,45679,35594,49831]
[null,"LiquiCal LL 230V/50Hz\nTemperature Range: -80°C to +110°C; Volume: 15,9 l; Weight: 91 kg"]
[null,"LIQUICAL LL 230V/50Hz",20100150,274072,null,36887,31869,45679,35594,49831]
[null,"LiquiCal HL 230V/50-60Hz\nTemperature Range: +35°C to +300°C; Volume: 15,9 l; Weight: 41 kg"]
[null,"LIQUICAL HL 230V/50-60Hz",20100142,135960,null,18299,15809,22660,17657,24720]
[]
[null,"ACCESSORIES"]
[null,"FIXTURES AND HOLDERS FOR TS PRO LOGGERS"]
[null,"Fixture for LiquiCal SL/HL/LL incl. stand & holder for 10 std. loggers"]
[null,"FIXTURE, COMPLETE F. 10 STD.",20000054,5069,null,682,589,845,658,922]
[null,"Fixture for LiquiCal SL/HL/LL,  incl. stand & holder for 16 miniloggers"]
[null,"FIXTURE, COMPLETE F. 16 MINIL",20000048,5069,null,682,589,845,658,922]
[null,"Additional holder for 10 std. loggers"]
[null,"ADD. HOLDER f.10 STD. LOGGER",20000072,2762,null,372,321,460,359,502]
[null,"Additional holder for 16 miniloggers"]
[null,"ADD. HOLDER f.16 MINILOGGERS",20000073,2762,null,372,321,460,359,502]
[null,"Additional holder for 20 microloggers"]
[null,"ADD. HOLDER f.20 MICROLOGGER",20000074,2762,null,372,321,460,359,502]
[null,"FIXTURES AND HOLDERS FOR EVP PROBES"]
[null,"Insert for LiquiCal SL, HL & LL. \nHolds 16 STC probes, and 1 ETS Temperature Standard (16 x ø5 x 300 mm, 1 x ø7 x 300 mm)"]
[null,"INSERT FOR LIQUICAL SL HL LL",20000104,11170,null,1503,1299,1862,1451,2031]
[null,"Insert for LiquiCal SL,HL & LL.\nHolds 16 probes SSA and ETS Temperature Standard (16 pcs ø 8/2.5 x 305 mm) , 1 pcs ø7.6 x 60 (open tube)"]
[null,"INSERT FOR LIQUICAL SL HL LL SSA PROBES",20000134,11170,null,1503,1299,1862,1451,2031]
[null,"LIQUICAL BATH LID"]
[null,"Lid with ø9mm center hole and 2 x 15mm perific holes for use with logger fixtures incl. handles"]
[null,"LIQUICAL BATH LID MOUNTED",20000147,2247,null,302,261,375,292,409]
[null,"LIQUICAL BATH DRIP TRAY"]
[null,"LiquiCal drip tray and exhaust system"]
[null,"LIQUICAL BATH DRIP TRAY",20000116,9161,null,1233,1065,1527,1190,1666]
[null,"USB ADAPTOR FOR ALL BATHS"]
[null,"RS232C to USB adaptor for connecting serial port of LiquiCal calibration bath to computer USB port"]
[null,"MOXA ADAPTOR USB-RS232/422/485",19000101,3261,null,439,379,544,424,593]
[]
[null,"BATH LIQUIDS"]
[]
[null,"Ellab Standard Oil (-30°C to +200°C), 1 Gallon = 3.8l",20000066,5482,null,738,637,914,712,997]
[null,"Ellab High-Temp Oil (80°C to +300°C), 1 Gallon = 3.8l",20000080,11151,null,1501,1297,1859,1448,2027]
[null,"Halocarbon low-temp oil (-80°C to +90°C), 1 Gallon = 3.8l",20000081,30373,null,4088,3532,5062,3945,5522]
[null,"For the liquids below: \nDangerous Goods - Transport price upon request"]
[null,"Syltherm XLT silicone thermal oil (-100°C to +25°C), 1 Gallon = 3.8l",20000129,5792,null,780,673,965,752,1053]
[null,"Ellab Low Temperature liquid (-80°C to +5°C), 1 Gallon = 3,8l",20000070,1984,null,267,231,331,258,361]

{"sheet":"Pressure Calibrator","index":3,"n_rows":25,"n_cols":10,"rows_kept":25,"cut":false,"hidden":false,"merged":[[0,8,1,9],[9,1,9,9],[14,1,14,9]]}
[null,"Ellab Calibration Solutions",null,null,null,null,null,null,{"$error":"#VALUE!"}]
[null,"Parts List: Pressure Calibrator"]
[null,"Calibration Pricing Ver. 02 - June 2026"]
[null,"1 January 2026 to 31 December 2026"]
[null,null,null,null,null,"DKK/€","DKK/£","DKK/$","DKK/CHF","DKK/Japan US"]
[null,null,null,null,null,7.43,8.6,6,7.7,5.5]
[null,"Description","Ellab Ordering\nCode","RRP DKK","Discount","RRP €","RRP £","RRP US$","RRP CHF","Japan US$"]
[null,"PRESSURE CALIBRATOR"]
[null,"PRESSURE CALIBRATOR"]
[null,"Pressure Calibrator with pump and carrying case.\nnVision base instrument with a 100 PSI G module and  an internal bar A module. Measuring range cover both 0 to 8 bar A and -1 to 7 bar G. Accuracy: +/-0,025 to 0,06%FS.\nSupplied with traceable calibration certificate (0 to 7 bar G), rubber boot, nVision software Pump, hose and adaptor 20003120 to fit Ellab pressure sensor part numbers 35127018/35127019 and Compact pressure logger 31191103/31191104"]
[null,"PRESSURE CALIBRATOR 100PSI WITH PUMP AND CARRYING CASE",20003100,60445,null,8135,7028,10074,7850,10990]
[null,"PRESSURE CALIBRATOR 300PSI WITH PUMP AND CARRYING CASE",20003101,60445,null,8135,7028,10074,7850,10990]
[]
[null,"CALIBRATION"]
[null,"nVision: Calibration in standard points."]
[null,"NVISION STD CAL NV/F +AFAL",20003000,4822,null,649,561,804,626,877]
[null,"NVISION 17025 STD CAL NV/H + AFAL",20003001,5630,null,758,655,938,731,1024]
[]
[null,"ACCESSORIES FOR PRESSURE CALIBRATOR"]
[null,"Adaptor for Pressure Calibrator (1st Gen pressure sensor)"]
[null,"PRESSURE CALIBRATOR HOSE ADAPTOR 1ST GEN",20003110,3381,null,455,393,564,439,615]
[null,"Adaptor for Pressure Calibrator (2nd Gen pressure sensor)"]
[null,"PRESSURE CALIBRATOR HOSE ADAPTOR 2ND GEN",20003120,3381,null,455,393,564,439,615]
[null,"Adaptor for Pressure Calibrator (E-Val Flex/ E-Val Pro pressure sensor)"]
[null,"PRESSURE CALIBRATOR HOSE ADAPTOR EVF DIG PRS SENSO",20003130,3381,null,455,393,564,439,615]

{"sheet":"Cal EQ - Rental","index":4,"n_rows":24,"n_cols":10,"rows_kept":24,"cut":false,"hidden":false,"merged":[[22,1,22,9],[0,8,1,9],[9,1,9,9],[20,1,20,9],[10,1,10,9],[19,1,19,9]]}
[null,"Ellab Calibration Solutions",null,null,null,null,null,null,{"$error":"#VALUE!"}]
[null,"Parts List: Rental"]
[null,"Calibration Pricing Ver. 02 - June 2026"]
[null,"1 January 2026 to 31 December 2026"]
[null,null,null,null,null,"DKK/€","DKK/£","DKK/$","DKK/CHF","DKK/Japan US"]
[null,null,null,null,null,7.43,8.6,6,7.7,5.5]
[null,"Description","Ellab Ordering\nCode","RRP DKK","Discount","RRP €","RRP £","RRP US$","RRP CHF","Japan US$"]
[null,"ELLAB TEMPERATURE STANDARD"]
[null,"ETS"]
[null,"All prices are per month"]
[null,"ETS 25 Standard\nSensor lenght 300mm\nProbe 100 Ohm\nUSB/PoE connection.\nIncl. Accredited Calibration Certificate and Suitecase.\nTemperature Range: -196 °C to 420 °C\nAccuracy: +/- 0.025 °C"]
[null,"1-Month Rental: ETS 25 Temp Standard (-196 to 420C)",29192000,5656,null,761,658,943,735,1028]
[null,"MANDATORY AS FOUND CALIBRATION AFTER RETURN"]
[null,"Accredited Calibration Certificate for ETS 25 Calibration points:  -196, -50,  0, +150, +420°C "]
[null,"CALIBRATION CERTIFICATE ETS 25",20000097,8796,null,1184,1023,1466,1142,1599]
[null,"Factory verification/comparison with other ETS TMP (3 std. points)"]
[null,"1-Month Rental: Mandatory As found ETS TMP Calibration",29900097,2966,null,399,345,494,385,539]
[]
[null,"DRY BLOCK"]
[null,"All prices are per month"]
[null,"RTC 159A Temperature Dry Block Model without Input option.\nTemperature range : -100 to +155°C\nWeight : 15.2 Kg\n115-230 V/50-60 Hz\nIncluding Carrying Case and Insert (16.5 kg)\nInsert for RTC 159 with hole dimensions of 24 x ø2.8 mm + 1 x ø6.55 mm (ETS) incl. insulation plug"]
[null,"1-Month Rental: RTC-159 Dryblock Calibrator w/ Insert -100C to +155C",29159000,22427,null,3018,2608,3738,2913,4078]
[null,"PTC 425A Temperature Dry Block Model without Input option.\nTemperature range : +33 to +425°C\nWeight : 8.2 Kg\n115-230 V/50-60 Hz\nIncluding Carrying Case and Insert with hole dimensions of 16 x ø2.8 + 1 x ø6.55 mm (ETS) without insulation plug."]
[null,"1-Month Rental: PTC-425 Dryblock Calibrator w/ Insert +33C to +425C",29425000,11220,null,1510,1305,1870,1457,2040]

{"sheet":"Version Control","index":5,"n_rows":7,"n_cols":9,"rows_kept":7,"cut":false,"hidden":false,"merged":[[0,7,1,8]]}
[null,null,null,null,null,null,null,{"$error":"#VALUE!"}]
[]
[]
[null,null,null,null,"Exchange Rates"]
[null,"Version","Release Date","Notes","DKK/€","DKK/£","DKK/$","DKK/CHF","DKK/Japan US"]
[null,1,"January 23, 2026","First version in new format",7.43,8.6,6,7.7,5.5]
[null,2,"June 04, 2026","Dry Blocks and Baths added"]