{"text_format":"1","workbook":"xlsx","n_sheets":10,"sheets":["TrackSense Pro","TrackSense LyoPro","TrackSense Lab","SteriSense","E-Val Pro","ValSuite 6","Val EQ - Rental","Calibration","Service and Documentation","Version Control"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":28,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TrackSense Pro","index":0,"n_rows":538,"n_cols":10,"rows_kept":538,"cut":false,"hidden":false,"merged":[[263,1,263,5],[60,1,60,9],[64,1,64,9],[67,1,67,9],[56,1,56,9],[196,1,196,2],[75,1,75,9],[16,1,16,9],[22,1,22,9],[27,1,27,9],[34,1,34,9],[48,1,48,9],[36,1,36,4],[39,1,39,4],[42,1,42,4],[45,1,45,4],[0,8,1,9],[537,1,537,9],[538,1,538,9],[272,1,272,6],[285,1,285,9],[287,1,287,9],[305,1,305,9],[307,1,307,9],[309,1,309,9],[317,1,317,9],[319,1,319,9],[324,1,324,9],[349,1,349,2],[403,1,403,3],[426,1,426,4],[9,1,9,9]]}
[null,"Ellab Validation Solutions",null,null,null,null,null,null,{"$error":"#VALUE!"}]
[null,"Parts List: TrackSense Pro"]
[null,"Validation Pricing Ver. 03 - July 2026"]
[null,"15 July 2026 to 31 December 2026"]
[null,null,null,null,null,"DKK/€","DKK/£","DKK/$","DKK/CHF","DKK/Japan US"]
[null,null,null,null,null,7.43,8.6,6,7.7,5.5]
[null,"Description","Ellab Ordering\nCode","RRP DKK","Discount","RRP €","RRP £","RRP US$","RRP CHF","Japan US$"]
[null,"TRACKSENSE PRO 3.1G MULTI READER STATION AND SOFTWARE"]
[null,"VALSUITE PRO"]
[null,"Requires ValSuite 3.1 or later version\nAll systems include: \n- ValSuite Software on USB key, USB Cable, Power Supply, LAN Connection, Sealant, Sensor Removal Tool, Carrying Case and Accessory Box\n- The ValSuite Pro Software include license for 2 Computers. The software is validated, 21 CFR part 11 compliant and developed according to GAMP.\n- The installation USB key includes user's manual on hardware and software. "]
[null,"TrackSense Pro Multi Reader Station for 4 Pro/Basic Loggers and ValSuite Pro Software",31188100,80265,null,10803,9333,13378,10424,14594]
[null,"TrackSense Pro Multi Reader Station for 4 Compact/Frigo Loggers and ValSuite Pro Software",31188113,80265,null,10803,9333,13378,10424,14594]
[null,"TrackSense Pro Multi Reader Station for 4 Mini Loggers and ValSuite Pro Software",31188104,80265,null,10803,9333,13378,10424,14594]
[null,"TrackSense Pro Multi Reader Station for 4 Micro Loggers and ValSuite Pro Software",31188107,80265,null,10803,9333,13378,10424,14594]
[null,"TrackSense Pro Multi Reader Station for 4 Frigo UX Sky Loggers and ValSuite Pro Software",31188114,80265,null,10803,9333,13378,10424,14594]
[null,"VALSUITE PLUS"]
[null,"Requires ValSuite 3.1 or later version\nAll systems include: \n- ValSuite Software on USB key, USB Cable, Power Supply, LAN Connection, Sealant, Sensor Removal Tool, Carrying Case and Accessory Box\n- ValSuite Plus Software including license for 2 Computers.\n- The installation USB key includes user's manual on hardware and software. "]
[null,"TrackSense Pro Multi Reader Station for 4 Pro/Basic Loggers and ValSuite Plus Software",31188201,57730,null,7770,6713,9622,7497,10496]
[null,"TrackSense Pro Multi Reader Station for 4 Compact/Frigo Loggers and ValSuite Plus Software",31188213,57730,null,7770,6713,9622,7497,10496]
[null,"TrackSense Pro Multi Reader Station for 4 Mini Loggers and ValSuite Plus Software",31188202,57730,null,7770,6713,9622,7497,10496]
[null,"TrackSense Pro Multi Reader Station for 4 Micro Loggers and ValSuite Plus Software",31188206,57730,null,7770,6713,9622,7497,10496]
[null,"VALSUITE MEDICAL"]
[null,"Requires ValSuite 3.1 or later version\nAll systems include: \n- ValSuite Software on USB key, USB Cable, Power Supply, LAN Connection, Sealant, Sensor Removal Tool, Carrying Case and Accessory Box\n- ValSuite Medical Software including license for 2 Computers. For hospitals only (documentation required). \n- The installation USB key includes user's manual on hardware and software. "]
[null,"TrackSense Pro Multi Reader Station for 4 Pro/Basic Loggers and ValSuite Medical Software",31188203,37581,null,5058,4370,6264,4881,6833]
[null,"TrackSense Pro Multi Reader Station for 4 Compact/Frigo Loggers and ValSuite Medical Software",31187204,37581,null,5058,4370,6264,4881,6833]
[null,"TrackSense Pro Multi Reader Station for 4 Mini Loggers and ValSuite Medical Software",31188205,37581,null,5058,4370,6264,4881,6833]
[null,"VALSUITE BASIC"]
[null,"Requires ValSuite 3.1 or later version\nAll systems include: \n- ValSuite Software on USB key, USB Cable, Power Supply, LAN Connection, Sealant, Sensor Removal Tool, Carrying Case and Accessory Box\n- ValSuite Basic Software including license for 2 Computers.\n- The installation USB key includes user's manual on hardware and software. "]
[null,"TrackSense Pro Multi Reader Station for 4 Pro/Basic Loggers and ValSuite Basic Software",31188300,37581,null,5058,4370,6264,4881,6833]
[null,"TrackSense Pro Multi Reader Station for 4 Compact/Frigo Loggers and ValSuite Basic Software",31188314,37581,null,5058,4370,6264,4881,6833]
[null,"TrackSense Pro Multi Reader Station for 4 Mini Loggers and ValSuite Basic Software",31188303,37581,null,5058,4370,6264,4881,6833]
[null,"TrackSense Pro Multi Reader Station for 4 Micro Loggers and ValSuite Basic Software",31188305,37581,null,5058,4370,6264,4881,6833]
[]
[null,"TRACKSENSE PRO 3.1G COMBO MULTI READER STATION AND SOFTWARE"]
[null,"Requires ValSuite 3.1 or later version\nAll systems include: \n- ValSuite Software on USB key, USB Cable, Power Supply, LAN Connection, Sealant, Sensor Removal Tool, Carrying Case and Accessory Box.\n- The installation USB key includes user's manual on hardware and software. \n- Please define logger slots as per section below."]
[null,"VALSUITE PRO"]
[null,"- The ValSuite Pro Software include license for 2 Computers. The software is validated, 21 CFR part 11 compliant and developed according to GAMP."]
[null,"TrackSense Pro COMBO Multi Reader Station for 4 loggers and ValSuite Pro Software",31188106,80265,null,10803,9333,13378,10424,14594]
[null,"VALSUITE PLUS"]
[null,"- ValSuite Plus Software including license for 2 Computers."]
[null,"TrackSense Pro COMBO Multi Reader Station for 4 loggers and ValSuite Plus Software",31188207,57730,null,7770,6713,9622,7497,10496]
[null,"VALSUITE MEDICAL"]
[null,"- ValSuite Medical Software including license for 2 Computers. For hospitals only (documentation required). "]
[null,"TrackSense Pro COMBO Multi Reader Station for 4 loggers and ValSuite Medical Software",31188209,37581,null,5058,4370,6264,4881,6833]
[null,"VALSUITE BASIC"]
[null,"- ValSuite Basic Software including license for 2 Computers. "]
[null,"TrackSense Pro COMBO Multi Reader Station for 4 loggers and ValSuite Basic Software",31188304,37581,null,5058,4370,6264,4881,6833]
[null,"MULTI READER STATION LOGGER SLOTS"]
[null,"Logger Slots for Combo Multi Reader Station"]
[null,"Pro/Basic logger slot for TS Pro Multi Combo Reader station",31188401,176,null,24,20,29,23,32]
[null,"Compact/Frigo logger slot for TS Pro Multi Combo Reader station",31188402,176,null,24,20,29,23,32]
[null,"Mini logger slot for TS Pro Multi Combo Reader station",31188403,176,null,24,20,29,23,32]
[null,"Micro logger slot for TS Pro Multi Combo Reader station",31188404,176,null,24,20,29,23,32]
[]
[null,"TRACKSENSE PRO SINGLE READER STATION AND SOFTWARE"]
[null,"VALSUITE PRO"]
[null,"All systems include: \n- ValSuite Software on USB key, USB Cable, Power Supply, LAN Connection, Sealant, Sensor Removal Tool, Carrying Case and Accessory Box\n- The ValSuite Pro Software include license for 2 Computers. The software is validated, 21 CFR part 11 compliant and developed according to GAMP.\n- The installation USB key includes user's manual on hardware and software. "]
[null,"TrackSense Pro Single Reader Station for 1 Pro/Basic Logger and ValSuite Pro Software",32183200,73234,null,9857,8516,12206,9511,13315]
[null,"TrackSense Pro Single Reader Station for 1 Compact/Frigo Logger and ValSuite Pro Software",32183203,73234,null,9857,8516,12206,9511,13315]
[null,"VALSUITE PLUS"]
[null,"All systems include: \n- ValSuite Software on USB key, USB Cable, Power Supply, LAN Connection, Sealant, Sensor Removal Tool, Carrying Case and Accessory Box\n- The ValSuite Plus Software include license for 2 Computers.\n- The installation USB key includes user's manual on hardware and software. "]
[null,"TrackSense Pro Single Reader Station for 1 Pro/Basic Logger and ValSuite Plus Software",32183110,50698,null,6823,5895,8450,6584,9218]
[null,"TrackSense Pro Single Reader Station for 1 Compact/Frigo Logger and ValSuite Plus Software",32183113,50698,null,6823,5895,8450,6584,9218]
[null,"VALSUITE MEDICAL"]
[null,"All systems include: \n- ValSuite Software on USB key, USB Cable, Power Supply, LAN Connection, Sealant, Sensor Removal Tool, Carrying Case and Accessory Box\n- The ValSuite Medical Software include license for 2 Computers. For hospitals only (documentation required).\n- The installation USB key includes user's manual on hardware and software. "]
[null,"TrackSense Pro Single Reader Station for 1 Pro/Basic Logger and ValSuite Medical Software",32183114,30342,null,4084,3528,5057,3941,5517]
[null,"VALSUITE BASIC"]
[null,"All systems include: \n- ValSuite Software on USB key, USB Cable, Power Supply, LAN Connection, Sealant, Sensor Removal Tool, Carrying Case and Accessory Box\n- The ValSuite Basic Software include license for 2 Computers.\n- The installation USB key includes user's manual on hardware and software. "]
[null,"TrackSense Pro Single Reader Station for 1 Pro/Basic Logger and ValSuite Basic Software",32183100,30342,null,4084,3528,5057,3941,5517]
[null,"TrackSense Pro Single Reader Station for 1 Compact/Frigo Logger and ValSuite Basic Software",32183103,30342,null,4084,3528,5057,3941,5517]
[null,"TrackSense Pro Single Reader Station for 1 Mini Logger and ValSuite Basic Software",32183102,30342,null,4084,3528,5057,3941,5517]
[null,"TrackSense Pro Single Reader Station for 1 Micro Logger and ValSuite Basic Software",32183101,30342,null,4084,3528,5057,3941,5517]
[]
[null,"TRACKSENSE PRO 3.1G MULTI READER STATION WITHOUT SOFTWARE"]
[null,"TRACKSENSE PRO MULTI READER STATION"]
[null,"Requires ValSuite 3.1 or later version\nAll systems include: \n- USB Cable, Power Supply, LAN Connection, Sealant, Sensor Removal Tool, Carrying Case and Accessory Box.\n- The installation USB key includes user's manual on hardware and software.\n- For Existing Customers Only. "]
[null,"TrackSense Pro Multi Reader Station for 4 Pro/Basic Loggers without Software",31188101,37581,null,5058,4370,6264,4881,6833]
[null,"TrackSense Pro Multi Reader Station for 4 Compact/Frigo Loggers without Software",31188102,37581,null,5058,4370,6264,4881,6833]
[null,"TrackSense Pro Multi Reader Station for 4 Mini Loggers without Software",31188103,37581,null,5058,4370,6264,4881,6833]
[null,"TrackSense Pro Multi Reader Station for 4 Micro Loggers without Software",31188108,37581,null,5058,4370,6264,4881,6833]
[null,"TRACKSENSE PRO COMBO MULTI READER STATION"]
[null,"TrackSense Pro COMBO Multi Reader Station for 4 loggers without Software",31188105,37581,null,5058,4370,6264,4881,6833]
[]
[null,"EXPANSION MODULES AND SKY OPTIONS"]
[null,"EXPANSION MODULES"]
[null,"Requires ValSuite 3.1 or later"]
[null,"TrackSense Pro Multi Expansion Module for 4 Pro/Basic Loggers",31187030,14315,null,1927,1665,2386,1859,2603]
[null,"TrackSense Pro Multi Expansion Module for 4 Compact/Frigo Loggers",31187012,14315,null,1927,1665,2386,1859,2603]
[null,"TrackSense Pro Multi Expansion Module for 4 Mini Loggers",31187011,14315,null,1927,1665,2386,1859,2603]
[null,"TrackSense Pro Multi Expansion Module for 4 Micro Loggers",31187013,14315,null,1927,1665,2386,1859,2603]
[null,"SKY OPTIONS"]
[]
[null,"Sky Access Point incl. USB and carrying case",31186000,38805,null,5223,4512,6468,5040,7055]
[null,"Sky Remote Antenna ø7 x 500 mm with 3 m cable",31190702,5152,null,693,599,859,669,937]
[null,"ACCESSORIES"]
[]
[null,"Supporting logger plate for multi reader station",35900027,625,null,84,73,104,81,114]
[null,"Ethernet relay for I/O control",35900040,5020,null,676,584,837,652,913]
[null,"Power Supply, required when using more than one Access Point in setup"]
[null,"Power Supply for Access Point, 12 V/1A DC (100-240 VAC)",25320005,770,null,104,90,128,100,140]
[]
[null,"MICRO DATA LOGGER"]
[null,"DATA LOGGERS"]
[null,"Logger incl. sensor and 2 batteries\nStandard Calibration Points are: 0, 60, 90, 120, 140°C\nRigid Sensor, sensor diameter 2,0 mm and measuring point 3 mm from tip"]
[null,"TS Micro Logger -20 to +140°C, incl. 10 mm single rigid sensor, no thread",31196210,20539,null,2764,2388,3423,2667,3734]
[null,"TS Micro Logger -20 to +140°C, incl. non-standard single rigid sensor, with thread","311962XX",24649,null,3317,2866,4108,3201,4482]
[null,"TS Micro Pressure/Temperature Logger, 10 mbar to 6 bar abs. Including internal temperature sensor",31195200,32020,null,4310,3723,5337,4158,5822]
[null,"BATTERIES"]
[null,"Battery for TSP Micro Logger\nNote: Dangerous Goods fee might apply when shipping batteries"]
[null,"TSP MICRO BATTERY, 1 set=2 pcs.",35500001,205,null,28,24,34,27,37]
[null,"TSP MICRO BATTERY, 5 sets = 10 pcs.",35500010,784,null,106,91,131,102,143]
[null,"TSP MICRO BATTERY, 50 sets = 100 pcs.",35500100,6206,null,835,722,1034,806,1128]
[null,"O-RINGS"]
[null,"O-ring for TSP Micro 1st gen., set of 10 pcs.",35900011,139,null,19,16,23,18,25]
[null,"O-ring for TSP Micro 2nd gen., set of 10 pcs.",35900022,184,null,25,21,31,24,33]
[]
[null,"MINI DATA LOGGER"]
[null,"DATA LOGGERS"]
[null,"Logger incl. sensor and 3 batteries\nStandard Calibration Points are: 0, 60, 90, 120, 140°C\nRigid Sensor, sensor diameter 2 mm and measuring point 3 mm from tip"]
[null,"TS Mini Logger 2 GEN, 0 to +140°C, built in sensor (0 mm), no thread",35211000,20539,null,2764,2388,3423,2667,3734]
[null,"TS Mini Logger 2 GEN, 0 to +140°C, incl 10 mm single rigid sensor, no thread",35221010,20539,null,2764,2388,3423,2667,3734]
[null,"TS Mini Logger 2 GEN, 0 to +140°C, incl 25 mm single rigid sensor, with thread",35221025,20544,null,2765,2389,3424,2668,3735]
[null,"TS Mini Logger 2 GEN, 0 to +140°C, incl 35 mm single rigid sensor, with thread",35221035,20539,null,2764,2388,3423,2667,3734]
[null,"TS Mini Logger 2 GEN, 0 to +140°C, incl 40 mm single rigid sensor, with thread",35221040,20539,null,2764,2388,3423,2667,3734]
[null,"TS Mini Logger 2 GEN, 0 to +140°C, incl 50 mm single rigid sensor, with thread",35221050,20539,null,2764,2388,3423,2667,3734]
[null,"TS Mini Logger 2 GEN, 0 to +140°C, incl 75 mm single rigid sensor, with thread",35221075,20539,null,2764,2388,3423,2667,3734]
[null,"TS Mini Logger 2 GEN, 0 to +140°C, incl 100 mm single rigid sensor, with thread",35221100,20539,null,2764,2388,3423,2667,3734]
[null,"TS Mini Logger 2 GEN, 0 to +140°C, incl. non-standard single rigid sensor, with thread","35221XXX",24649,null,3317,2866,4108,3201,4482]
[null,"BATTERIES"]
[null,"Battery for TSP Mini & TS Lab Mini Loggers\nNote: Dangerous Goods fee might apply when shipping batteries"]
[null,"TSP MINI BATTERY, 1 pc.",35300001,114,null,15,13,19,15,21]
[null,"TSP MINI BATTERY, pack of 10 pcs.",35300010,784,null,106,91,131,102,143]
[null,"TSP MINI BATTERY, pack of 100 pcs.",35300100,6206,null,835,722,1034,806,1128]
[null,"O-RING"]
[null,"O-ring for TSP Mini Logger, set of 10 pcs.",35900010,139,null,19,16,23,18,25]
[]
[null,"COMPACT DATA LOGGER"]
[null,"DATA LOGGERS WITH RIGID SENSOR"]
[null,"Logger incl. sensor and 1 battery\nStandard Calibration points are: 0, 60, 90, 120, 140°C\nRigid Sensor with thread, sensor diameter 2,0 mm and measuring point 3 mm from tip"]
[null,"TS Compact Logger -30 to +140 °C, incl 35 mm single rigid sensor",31191202,14572,null,1961,1694,2429,1892,2649]
[null,"TS Compact Logger -30 to +140 °C, incl 50 mm single rigid sensor",31191203,14572,null,1961,1694,2429,1892,2649]
[null,"TS Compact Logger -30 to +140 °C, incl 75 mm single rigid sensor",31191204,14572,null,1961,1694,2429,1892,2649]
[null,"TS Compact Logger -30 to +140 °C, incl. 100 mm single rigid sensor",31191205,14572,null,1961,1694,2429,1892,2649]
[null,"DATA LOGGERS WITH SEMIFLEX SENSOR"]
[null,"Logger incl. sensor and 1 battery\nStandard Calibration points are: 0, 60, 90, 120, 140°C\nSingle SemiFlex Sensor, sensor diameter 1,5 mm and measuring point 3 mm from tip"]
[null,"TS Compact Logger -30 to +140 C, 30 cm single SemiFlex sensor",31191270,19706,null,2652,2291,3284,2559,3583]
[null,"TS Compact Logger -30 to +140 C, 50 cm single SemiFlex sensor",31191271,19706,null,2652,2291,3284,2559,3583]
[null,"DATA LOGGERS WITH SMARTFLEX SENSOR"]
[null,"Logger incl. sensor and 1 battery\nStandard Calibration Points are: 0, 60, 90, 120, 140°C\nSmartFlex Sensor, sensor diameter 1,8 mm and measuring point 3 mm from tip"]
[null,"TS Compact Logger -30 to +140 C, 30 cm single SmartFlex sensor",31191250,17993,null,2422,2092,2999,2337,3271]
[null,"TS Compact Logger -30 to +140 C, 50 cm single SmartFlex sensor",31191251,17993,null,2422,2092,2999,2337,3271]
[null,"DATA LOGGERS WITH PRESSURE SENSOR"]
[null,"Logger incl. sensor and 1 battery\nStandard Calibration Points are: 0, 60, 90, 120, 140°C\nMeasuring point 3 mm from tip"]
[null,"TS Compact Pressure Logger, 6 bar",31191103,22871,null,3078,2659,3812,2970,4158]
[null,"TS Compact Pressure Logger 6 bar, combined temperature & pressure",31191104,26865,null,3616,3124,4478,3489,4885]
[null,"BATTERIES"]
[null,"High Performance Battery for Pro, Basic, Compact and Lab Loggers\nNote: Dangerous Goods fee might apply when shipping batteries"]
[null,"TSP BATTERY with Activator",35900050,1037,null,140,121,173,135,189]
[null,"TSP BATTERY without Activator",35900051,777,null,105,90,130,101,141]
[null,"High Performance Battery - Only for Compact Ultra X and TS Pro XL Loggers\nNote: Dangerous Goods fee might apply when shipping batteries"]
[null,"TSP Battery 150L with Activator",35900055,1037,null,140,121,173,135,189]
[null,"TSP Battery 150L without Activator",35900056,777,null,105,90,130,101,141]
[null,"O-RINGS"]
[null,"O-ring for TSP Compact, set of 10 pcs.",35900019,139,null,19,16,23,18,25]
[]
[null,"FRIGO DATA LOGGER"]
[null,"DATA LOGGERS - INTERNAL AND RIGID SENSOR"]
[null,"Logger incl. sensor and 1 battery\nStandard Calibration Points are: -90, -30, 0, 40 and 85°C\nRigid Sensor: Sensor diameter 2mm and measuring point 3 mm from tip\nQuantity discount: 5% at more than 10 units, 10 % at more than 25 units, 15% at more than 50 units"]
[null,"TS Frigo logger -90 to +85 °C, with LED indicator and internal sensor",31191500,12216,null,1644,1420,2036,1586,2221]
[null,"TS Frigo logger -90 to +85 °C, with LED indicator and 35mm rigid sensor",31191501,12650,null,1703,1471,2108,1643,2300]
[null,"DATA LOGGERS WITH SEMIFLEX SENSOR"]
[null,"Logger incl. sensor and 1 battery\nStandard Calibration Points are: -90, -30, 0, 40 and 85°C\nSemiFlex Sensor, measuring point 3 mm from tip\nQuantity discount: 5% at more than 10 units, 10 % at more than 25 units, 15% at more than 50 units"]
[null,"TS Frigo Logger -90 to +85 C, 30 cm single SemiFlex sensor, ø1,5mm",31191570,17770,null,2392,2066,2962,2308,3231]
[null,"TS Frigo Logger -90 to +85 C, 50 cm single SemiFlex sensor, ø1,5mm",31191571,17770,null,2392,2066,2962,2308,3231]
[null,"TS Frigo Logger -90 to +85 C, without LED indicator, 30 cm single SemiFlex sensor, ø2,0mm",31191572,15640,null,2105,1819,2607,2031,2844]
[null,"DATA LOGGERS WITH SMARTFLEX SENSOR"]
[null,"Logger incl. sensor and 1 battery\nStandard Calibration Points are: -90, -30, 0, 40 and 85°C\nSmartFlex Sensor, sensor diameter 1,8mm and measuring point 3 mm from tip\nQuantity discount: 5% at more than 10 units, 10 % at more than 25 units, 15% at more than 50 units"]
[null,"TS Frigo Logger -90 to +85 C, 30 cm single SmartFlex sensor",31191550,16055,null,2161,1867,2676,2085,2919]
[null,"TS Frigo Logger -90 to +85 C, 50 cm single SmartFlex sensor",31191551,16055,null,2161,1867,2676,2085,2919]
[null,"BATTERIES"]
[null,"High performance battery for TS Frigo Loggers, -90 to +85°C\nNote: Dangerous Goods fee might apply when shipping batteries"]
[null,"TS FRIGO BATTERY with Activator",35900060,696,null,94,81,116,90,127]
[null,"TS FRIGO BATTERY without Activator",35900061,465,null,63,54,78,60,85]
[null,"O-RINGS"]
[null,"O-ring for TS Frigo, set of 10 pcs.",35900021,139,null,19,16,23,18,25]
[]
[null,"FRIGO UX SKY DATA LOGGER"]
[null,"DATA LOGGERS - INTERNAL AND RIGID SENSOR"]
[null,"Logger with integrated sky module incl. sensor and 2 batteries\nStandard Calibration Points are: -90, -40, 0, 60, 140°C\nRigid Sensor: Sensor diameter 2mm and measuring point 3 mm from tip"]
[null,"TS Frigo UX SKY Logger with 35mm Rigid Sensor","31191210UX",19640,null,2643,2284,3273,2551,3571]
[null,"TS Frigo UX SKY Logger with 100mm Rigid Sensor","31191213UX",19640,null,2643,2284,3273,2551,3571]
[null,"DATA LOGGERS WITH SEMIFLEX SENSOR"]
[null,"Logger with integrated sky module incl. sensor and 2 batteries\nStandard Calibration Points are: -90, -40, 0, 60, 140°C\nSemiFlex Sensor: Sensor diameter 1.5mm and measuring point 3 mm from tip"]
[null,"TS Frigo UX SKY Logger with 30cm SemiFlex Sensor","31191214UX",22655,null,3049,2634,3776,2942,4119]
[null,"TS Frigo UX SKY Logger with 50cm SemiFlex Sensor","31191215UX",22655,null,3049,2634,3776,2942,4119]
[null,"DATA LOGGERS WITH PRESSURE SENSOR"]
[null,"Logger with integrated sky module incl. sensor and 2 batteries\nStandard Calibration Points: Temperature: 25, 70, 90, 120, 140°C, Pressure: 50, 1000, 3000, 4000 mbar\nMeasuring point 3 mm from tip"]
[null,"TS Frigo UX SKY Logger Pressure/Temperature",31191110,27182,null,3658,3161,4530,3530,4942]
[null,"BATTERIES"]
[null,"High Performance Battery\nNote: Dangerous Goods fee might apply when shipping batteries"]
[null,"TSP BATTERY with Activator",35900050,1037,null,140,121,173,135,189]
[null,"TSP BATTERY without Activator",35900051,777,null,105,90,130,101,141]
[null,"O-RINGS"]
[null,"O-ring for TS Frigo UX Sky, Set of 10 pcs.",35900075,183,null,25,21,31,24,33]
[]
[null,"TRACKSENSE PRO DATA LOGGER"]
[null,"DATA LOGGERS"]
[null,"Logger without sensor. 1 battery included\nAll loggers are ATEX certified. "]
[null,"TS PRO X LOGGER 3G, ATEX Code: Ex ia IIC T3 Ga, -60 to +105°C"]
[null,"TS PRO X LOGGER 3G, -80 to +150°C",31192103,21258,null,2861,2472,3543,2761,3865]
[null,"TS PRO LOGGER 3G, ATEX Code: Ex ia IIC T3 Ga, -50 to +105°C"]
[null,"TS PRO LOGGER 3G, -50 to +150°C",31192003,18749,null,2523,2180,3125,2435,3409]
[null,"TS PRO BASIC LOGGER 3G:  Ex ia IIC T3 Ga, -30 to +105°C\nQuantity discount: 10% at more than 25 units, 15% at more than 50 units"]
[null,"TS PRO BASIC LOGGER 3G, -30 to +105°C",31191003,11492,null,1547,1336,1915,1492,2089]
[null,"SKY MODULE"]
[null,"ATEX Code: Ex ia IIC T3 Ga, -60 to +105°C"]
[null,"SKY MODULE PRO 3G",31190501,5953,null,801,692,992,773,1082]
[null,"BATTERIES"]
[null,"High Performance Battery for Pro, Basic, Compact and Lab Loggers\nNote: Dangerous Goods fee might apply when shipping batteries"]
[null,"TSP BATTERY with Activator",35900050,1037,null,140,121,173,135,189]
[null,"TSP BATTERY without Activator",35900051,777,null,105,90,130,101,141]
[null,"High Performance Battery for Cold Applications\nNote: Dangerous Goods fee might apply when shipping batteries"]
[null,"TSP Battery COLD with Activator",35900053,1037,null,140,121,173,135,189]
[null,"TSP Battery COLD without Activator",35900054,777,null,105,90,130,101,141]
[null,"O-RINGS"]
[null,"O-ring for TSP Logger, set of 10 pcs.",35900007,232,null,31,27,39,30,42]
[]
[null,"TRACKSENSE PRO X LONG EDITION"]
[null,"DATA LOGGERS"]
[null,"Logger without sensor. 1 battery included\nPro XL Loggers are ATEX certified\nATEX Code: Ex ia IIC T3 Ga, -55 to +105°C"]
[null,"TS PRO XL LOGGER 3G, -80 to +150°C",31192203,23201,null,3123,2698,3867,3013,4218]
[null,"SKY MODULE"]
[null,"ATEX Code: Ex ia IIC T3 Ga, -55 to +105°C"]
[null,"SKY MODULE PRO XL 3G",31190523,6218,null,837,723,1036,808,1131]
[null,"BATTERIES"]
[null,"High Performance Battery - Only for Compact Ultra X and TS Pro XL Loggers\nNote: Dangerous Goods fee might apply when shipping batteries"]
[null,"TSP Battery 150L with Activator",35900055,1037,null,140,121,173,135,189]
[null,"TSP Battery 150L without Activator",35900056,777,null,105,90,130,101,141]
[null,"O-RINGS"]
[null,"O-ring for TSP Logger, set of 10 pcs.",35900007,232,null,31,27,39,30,42]
[]
[null,"TRACKSENSE BASIC L"]
[null,"DATA LOGGERS"]
[null,"Logger without sensor. 1 battery included"]
[null,"TS PRO BASIC L LOGGER 3G, NOT ATEX, -30 to +85°C",31191093,13431,null,1808,1562,2239,1744,2442]
[null,"BATTERIES"]
[null,"High performance battery for TS Pro Basic L Loggers, -30 to +85C\nNote: Dangerous Goods fee might apply when shipping batteries"]
[null,"TS PRO BASIC L BATTERY with Activator",35900080,696,null,94,81,116,90,127]
[null,"TS PRO BASIC L BATTERY without Activator",35900081,465,null,63,54,78,60,85]
[null,"O-RINGS"]
[null,"O-ring for TSP Logger, set of 10 pcs.",35900007,232,null,31,27,39,30,42]
[]
[null,"TEMPERATURE SENSORS FOR TRACKSENSE PRO"]
[null,"INTERNAL AND RIGID SINGLE SENSORS"]
[null,"Standard Calibration Points are: 0, 60, 90, 120, 140°C\nSensor diameter 2mm and measuring point 3 mm from tip\nSensors longer than 10 mm are standard with thread."]
[null,"TS PRO Single Internal Sensor",35121000,4638,null,624,539,773,602,843]
[null,"TS PRO Single Rigid Sensor, 10 mm, rounded point",35121010,4638,null,624,539,773,602,843]
[null,"TS PRO Single Rigid Sensor, 25 mm, rounded point",35121025,4638,null,624,539,773,602,843]
[null,"TS PRO Single Rigid Sensor, 50 mm, rounded point",35121050,4638,null,624,539,773,602,843]
[null,"TS PRO Single Rigid Sensor, 75 mm, rounded point",35121075,4638,null,624,539,773,602,843]
[null,"TS PRO Single Rigid Sensor, 100 mm, rounded point",35121100,4638,null,624,539,773,602,843]
[null,"TS PRO Single Rigid Sensor, 150 mm, rounded point",35121150,4638,null,624,539,773,602,843]
[null,"TS PRO Single Rigid Sensor, 200 mm, rounded point",35121200,4638,null,624,539,773,602,843]
[null,"Non-Standard Single Rigid Sensor, Please replace the required length in millimeters in the section with the XXX. (E.g. TPA20085TS = 85 mm electrode length)."]
[null,"TPA20XXXTS - TS PRO Non-Standard Single Rigid Sensor, rounded point","3512XXXX",5180,null,697,602,863,673,942]
[null,"RIGID DOUBLE SENSORS"]
[null,"Standard Calibration Points are: 0, 60, 90, 120, 140°C\nOne Product Sensor in various length and one 20 mm U-shaped ambient sensor.\nSensor diameter 2mm and measuring point 3 mm from tip\nSensors longer than 10 mm are standard with thread."]
[null,"TS PRO Double Rigid Sensor with 50 mm product sensor",35122701,6511,null,876,757,1085,846,1184]
[null,"TS PRO Double Rigid Sensor with 75mm product sensor ",35122703,6511,null,876,757,1085,846,1184]
[null,"TS PRO Double Rigid Sensor with 100 mm product sensor",35122702,6511,null,876,757,1085,846,1184]
[null,"TS PRO Double Rigid Sensor with 150 mm product sensor",351227100,6511,null,876,757,1085,846,1184]
[null,"TS PRO Double Rigid Sensor with 200 mm product sensor",35122782,6511,null,876,757,1085,846,1184]
[null,"Double Rigid Sensor, Rigid product sensor & a rigid ambient sensor.\nPlease compose your type designation as follows: Z = A (rounded point), N (conic point), K (sharp point), R (round no thread), S (conic no thread), C (sharp, no thread).\nXXX = electrode length of product sensor in mm.\nTS = rigid double sensor\nQuantity discount: 20% at 10 or more units. "]
[null,"TPZ20XXXTSYYYLZZZ - TS PRO Double Rigid Sensor","351227XX",8138,null,1095,946,1356,1057,1480]
[null,"MULTIPOINT SENSORS"]
[null,"4 Measuring points. Sensor diameter 2,5mm with 10 mm distance between measuring points.\nSensors longer than 10 mm are standard with thread."]
[null,"TS PRO Single Rigid Muliti Point (4) 100 mm Sensor",35121910,19713,null,2653,2292,3286,2560,3584]
[null,"SMARTFLEX SENSORS"]
[null,"Min. length 20 cm, max. lenght 100 cm. Tolerance -0/+5 cm. Available in intervals of 10 cm.\nStandard Calibration Points are: 0, 60, 90, 120, 140°C\nSensor diameter 1,8 mm and measuring point 3 mm from tip. SmartFlex wire until 10 mm from tip.\nMax. temperature 140°C."]
[null,"TS PRO SmartFlex Single Sensor, 30 cm",35124527,7002,null,942,814,1167,909,1273]
[null,"TS PRO SmartFlex Single Sensor, 50 cm",35124526,7002,null,942,814,1167,909,1273]
[null,"TS PRO SmartFlex Single Sensor, 100 cm",35124529,8271,null,1113,962,1379,1074,1504]
[null,"TS PRO SmartFlex Double Sensor, 30 cm",35124935,12117,null,1631,1409,2020,1574,2203]
[null,"TS PRO SmartFlex Double Sensor, 50 cm",35124936,12117,null,1631,1409,2020,1574,2203]
[null,"TS PRO SmartFlex Double Sensor, 100 cm",35124937,15648,null,2106,1820,2608,2032,2845]
[null,"Combi Double sensor, with one rigid ambient sensor & one SmartFlex sensor. \nPlease replace Y and Z as follows: YYY = length of SmartFlex flexible 1.8 mm cable in centimeters (max. 70 cm). ZZZ = electrode length of ambient sensor in mm, min. 10 mm for 180° angled ambient sensor 30 mm\nQuantity discount: 20% at 10 or more units."]
[null,"TPT18L02TFRYYYUZZZ - TS PRO Combi Double Sensor","351248XX",14415,null,1940,1676,2403,1872,2621]
[null,"STAINLESS STEEL TIP\nTAJ25XXXC Rounded point with thread\nTNJ25XXXC Conical point with thread\nTKJ25XXXC Sharp point with thread\nTRJ25XXXC Round point, no thread\nTSJ25XXXC Conical point, no thread\nTCJ25XXXC Sharp point, no thread\nXXX = length of tip in mm, Tip min. 35 mm, max. 150 mm, diameter ø2,5 mm (standard)"]
[null,"STAINLESS STEELTIP FOR TPT TFR","359003XX",813,null,109,95,136,106,148]
[null,"RUGGED FLEXIBLE SENSORS"]
[null,"Standard Calibration Points are: 0, 60, 90, 120, 140°C\nSensor diameter 2,5 mm and measuring point 5 mm from tip. Flexible wire until 50 mm from tip.\nFlexible wire in various length "]
[null,"PTFE steel enforced sensor with ø2.5 x 30 mm rounded tip, no thread."]
[null,"TS PRO Rugged flexible sensor, no thread, 50 cm",35124000,8131,null,1094,945,1355,1056,1478]
[null,"TS PRO Rugged flexible sensor, no thread, 100 cm",35124001,8131,null,1094,945,1355,1056,1478]
[null,"PTFE steel enforced sensor with ø2.5 x 30 mm rounded tip and thread."]
[null,"TS PRO Rugged flexible sensor, thread, 50 cm",35124002,8131,null,1094,945,1355,1056,1478]
[null,"TS PRO Rugged flexible sensor, thread, 100 cm",35124003,8131,null,1094,945,1355,1056,1478]
[null,"SEMI FLEXIBLE SENSORS"]
[null,"Standard Calibration Points are: 0, 60, 90, 120, 140°C\nStainless steel flexible temperature sensor with ø1,5 mm rounded tip (only).\nSensor diameter 1,5 mm and measuring point 3 mm from tip.\nFlexible wire in various length "]
[null,"TS PRO Semi Flexible Single Sensor, 30 cm",351225322,7813,null,1052,908,1302,1015,1421]
[null,"TS PRO Semi Flexible Single Sensor, 50 cm",351225321,7813,null,1052,908,1302,1015,1421]
[null,"TS PRO Semi Flexible Double Sensor, 30 cm",351229692,15571,null,2096,1811,2595,2022,2831]
[null,"TS PRO Semi Flexible Double Sensor, 50 cm",351229691,15571,null,2096,1811,2595,2022,2831]
[null,"SEMI FLEXIBLE SENSORS"]
[null,"Standard Calibration Points are: 0, 60, 90, 120, 140°C\nMax. length 100 cm.\nSensor diameter 2,0 mm and measuring point 3 mm from tip."]
[null,"Semi Flexible Single Sensor, Stainless steel flexible temperature sensor.\nPlease replace X, Y and Z as follows:\nXXX = length of electrode in millimeters (min. length varies - see below)\nYYY = length of stainless steel flexible wire in centimeters\nZ = A (rounded point) 15 mm, N (conic point) 20 mm, K (sharp point) 20 mm, R (round no thread) 15 mm, S (conic no thread) 20 mm, C (sharp, no thread) 20 mm."]
[null,"TPZ20XXXSCYYY - TS PRO Semi Flexible Single Sensor","351225XX",8589,null,1156,999,1432,1115,1562]
[null,"Double Semi Flexible Sensor with two stainless steel flexible sensors.\nPlease compose your type designation as follows: Z = A (rounded point) 15 mm, N (conic point) 20 mm, K (sharp point) 20 mm, R (round no thread) 15 mm, S (conic no thread) 20 mm, C (sharp, no thread) 20 mm.\nXXX = electrode length of both sensors in mm, minimum lenght varies, see above\nDDC = flexible double sensor\nYYY = sensor 1 - length of stainless steel flexible wire in cm\nI = angle of 0° both sensors\nZZZ = sensor 2 - length of stainless steel flexible wire in cm\nAbove probes can also be delivered with ø3 mm electrodes. Please replace with e.g. TPA3\nQuantity discount: 20% at 10 or more units."]
[null,"TPZ20XXXDDCYYYIZZZ - TS PRO Double Semi Flexible Sensor","351229XX",19435,null,2616,2260,3239,2524,3534]
[null,"Double Rigid & Semi Flex Sensor with one rigid ambient sensor & one flexible product sensor.\nPlease compose your type designation as follows: Z = A (rounded point) 15 mm, N (conic point) 20 mm, K (sharp point) 20 mm, R (round no thread) 15 mm, S (conic no thread) 20 mm, C (sharp, no thread) 20 mm.\nXXX = electrode length of product sensor in mm, min. length varies (see above)\nDC = flexible rigid double sensor\nYYY = length of stainless steel flexible wire in cm\nI = angle of 0°  L = angle of 90°\nU = angle of 180°\nZZZ = electrode length of rigid ambient sensor in mm, min. 10 - for 180° angled ambient sensor 30n mm, min. 10 - for 180° angled ambient sensor 30 mm\nQuantity discount: 20% at 10 or more units. "]
[null,"TPZ20XXXDCYYYLZZZ - TS PRO Double Rigid & Semi Flex Sensor","351226XX",18506,null,2491,2152,3084,2403,3365]
[null,"HIGH TEMPERATURE SENSORS"]
[null,"Standard Calibration Points are: 0, 90, 160, 240, 360, 400°C.\nMinimum length of sensor 200 mm.\nSensor diameter ø2,0 x 12 mm. Measuring point 3 mm from tip.\nFlexible mineral insulated wires in various lengths, rounded point."]
[null,"TS PRO Single Flexible High Temperature Sensor, 30 cm",35123266,8768,null,1180,1020,1461,1139,1594]
[null,"TS PRO Single Flexible High Temperature Sensor, 50 cm",35123267,8768,null,1180,1020,1461,1139,1594]
[null,"TS PRO Double Flexible High Temperature Sensor, 30 cm",35122855,14548,null,1958,1692,2425,1889,2645]
[null,"TS PRO Double Flexible High Temperature Sensor, 50 cm",35122856,14548,null,1958,1692,2425,1889,2645]
[null,"Please replace XXX with the required length: XXX = length of flexible mineral insulated wire in cm"]
[null,"TPR20012THSXXX - TS PRO Single Flexible High Temperature Sensor","3512326X",10521,null,1416,1223,1754,1366,1913]
[null,"Please replace XXX with the required length: XXX = length of flexible mineral insulated wires in cm"]
[null,"TPR20012THDXXX - TS PRO Double Flexible High Temperature Sensor","351228XX",17459,null,2350,2030,2910,2267,3174]
[null,"LOW TEMPERATURE THERMOCOUPLE SENSOR"]
[null,"Operating range -80 to +62°C.\nStandard Calibration Points: -60, -30, 0, +30, +60°C."]
[null,"TS PRO TC sensor incl. 30 cm long Thermocouple",35123501,9016,null,1213,1048,1503,1171,1639]
[null,"Quantity discount: 20% at 5 units or more. 30 % at 10 units or more."]
[null,"TS PRO Thermocouple, 10 cm",35123521,444,null,60,52,74,58,81]
[null,"TS PRO Thermocouple, 30 cm",35123523,444,null,60,52,74,58,81]
[null,"TS PRO Thermocouple, 50 cm",35123525,487,null,66,57,81,63,89]
[null,"TS PRO Thermocouple, 100 cm",35123530,531,null,71,62,89,69,97]
[]
[null,"RELATIVE HUMIDITY SENSORS FOR TRACKSENSE PRO"]
[null,"SENSORS"]
[null,"Relative Humidity Sensor for EtO and Stability Chambers with PT1000. Accuracy +/- 2%.\nRequires ValSuite 5.2.0.10 or later."]
[null,"TS PRO Relative Humidity Sensor 5.2",35128013,7969,null,1073,927,1328,1035,1449]
[null,"TS PRO Double Temperature Dry & Wet Sensor",35126000,6511,null,876,757,1085,846,1184]
[null,"ACCESSORIES"]
[null,"Reservoir for Dry & Wet measurement",35126010,2661,null,358,309,444,346,484]
[null,"Fixture for Logger and Water reservoir",35126011,3475,null,468,404,579,451,632]
[]
[null,"PRESSURE SENSORS FOR TRACKSENSE PRO"]
[null,"SENSORS"]
[null,"Range: 0 to 8 bar\nStandard Calibration Points, 4 bar: 50, 1000, 3000, 4000 mbar\nStandard Calibration Points, 6 bar: 50, 1000, 3500, 6000 mbar\nStandard Calibration Points, 8 bar: 50, 1000, 3500, 6000, 8000 mbar"]
[null,"TS PRO Pressure Sensor, 4 bar, SKY Compatible",35127024,13417,null,1806,1560,2236,1742,2439]
[null,"TS PRO Pressure Sensor, 6 bar, SKY Compatible",35127018,13417,null,1806,1560,2236,1742,2439]
[null,"TS PRO Pressure Sensor, 8 bar, SKY Compatible",35127021,14835,null,1997,1725,2473,1927,2697]
[null,"Combined temperature & pressure. Sensor length 20 mm, no thread."]
[null,"TS PRO Pressure/Temperature Sensor, 4 bar, SKY Compatible",35127023,17338,null,2334,2016,2890,2252,3152]
[null,"TS PRO Pressure/Temperature Sensor, 6 bar, SKY Compatible",35127019,17338,null,2334,2016,2890,2252,3152]
[null,"ACCESSORIES"]
[null,"Pressure connection system for pressure sensor, without capillary tube (not suitable for prs/tmp sensor)"]
[null,"PAJ/TS PRO-PRESSURE SYSTEM",35510004,3665,null,493,426,611,476,666]
[]
[null,"BOWIE DICK SENSOR FOR TRACKSENSE PRO"]
[null,"For 121˚C and 134˚C.\nOnly for TS Pro, X and XL logger.\nRequires ValSuite 5.3 or later."]
[null,"TS PRO Bowie Dick Sensor. incl. PCD and protective adaptor",35127022,20472,null,2755,2380,3412,2659,3722]
[null,"Process Challenge Device (PCD)",35000500,2238,null,301,260,373,291,407]
[]
[null,"VACUUM SENSOR FOR TRACKSENSE PRO"]
[null,"Pressure Range: 0.001 to 100 mBar.\nTemperature Range: -80 to +140°C.\nRequires ValSuite 4.1.x or later."]
[null,"TS PRO Vacuum Sensor",35127900,23562,null,3171,2740,3927,3060,4284]
[]
[null,"CONDUCTIVITY SENSORS FOR TRACKSENSE PRO"]
[null,"Conductivity Sensor with combined temperature sensor.\nRange: 0-200 µS/cm or  200-2000 µS/cm.\nRequires ValSuite 3.0 or later"]
[null,"TS PRO Conductivity Sensor, 0-200",35132000,12210,null,1643,1420,2035,1586,2220]
[null,"TS PRO Conductivity Sensor, 200-2000",35132001,12210,null,1643,1420,2035,1586,2220]
[]
[null,"CO2 SENSORS FOR TRACKSENSE PRO"]
[null,"0-10% - Calibration Points: 0, 5, 7.5 and 10%\n0-20% - Calibration Points: 0, 5, 10, 15 and 20%\nRequires TSP Basic L Logger and No ATEX environment."]
[null,"TS PRO CO2 Sensor 2G, 0-10%",35127921,19510,null,2626,2269,3252,2534,3547]
[null,"TS PRO CO2 Sensor 2G, 0-20%",35127922,22440,null,3020,2609,3740,2914,4080]
[]
[null,"AUTOMARKER SENSOR FOR TRACKSENSE PRO"]
[]
[null,"TS PRO AM 2.6 AutoMarker Sensor",35131000,7851,null,1057,913,1309,1020,1427]
[]
[null,"THERMAL BARRIERS"]
[null,"THERMAL BARRIERS FOR SINGLE OR DOUBLE HIGH TEMPERATURE SENSOR"]
[null,"Material: Stainless Steel, Brushed\nSKY: Sky compatible"]
[null,"Diameter: ø35 mm x 150 mm, Max. 10 minutes at +400°C"]
[null,"TTB35-2 THERMAL BARRIER DBL., ø35 mm x 150 mm",25901503,14459,null,1946,1681,2410,1878,2629]
[null,"Diameter: ø64 mm x 150 mm. Max. 50 minutes at +400°C"]
[null,"TTB64-2 THERMAL BARRIER DBL., ø64 mm x 150 mm",25901502,11952,null,1609,1390,1992,1552,2173]
[null,"TTB64-2 THERMAL BARRIER SKY DBL., ø64 mm x 150 mm",25901514,13331,null,1794,1550,2222,1731,2424]
[null,"Diameter: ø85 mm x 175 mm. Max. 110 minutes at +400°C"]
[null,"TTB85-2 THERMAL BARRIER DBL., ø85 mm x 175 mm",25901529,19247,null,2590,2238,3208,2500,3499]
[null,"TTB85-2 THERMAL BARRIER SKY, ø85 mm x 175 mm",25901530,20804,null,2800,2419,3467,2702,3783]
[null,"Dimension: 40 x 40 x 153 mm. Max. 20 minutes at +400°C"]
[null,"TBS40-3 THERMAL BARRIER SQUARE, 40x40x153 mm",25901524,14472,null,1948,1683,2412,1879,2631]
[null,"TBS40-3 THERMAL BARRIER SKY SQUARE, 40x40x153 mm",25901525,15459,null,2081,1798,2577,2008,2811]
[null,"Dimension: 40 x 100 x 153 mm. Max. 40 minutes at 400 °C"]
[null,"TBF40-3 THERMAL BARRIER, 40x100x153 mm",25901520,15343,null,2065,1784,2557,1993,2790]
[null,"TBF40-3 THERMAL BARRIER SKY, 40x100x153 mm",25901521,16402,null,2208,1907,2734,2130,2982]
[null,"THERMAL BARRIERS FOR SINGLE RIGID HIGH TEMPERATURE SENSOR"]
[null,"Special thermal barrier in PTFE for single rigid sensors with a max diameter of ø2mm.\nDiameter: ø65 x 86 mm. Max. temperature +200°C, Max. 60 minutes at +170°C"]
[null,"TTB65 THERMAL BARRIER, PTFE, ø65 x 86 mm, sensor ø2mm  ",25901507,7530,null,1013,876,1255,978,1369]
[null,"SKY THERMAL BARRIER KIT"]
[null,"Sky Thermal Barrier Kit for TTB64, TTB80, and TTB85"]
[null,"SKY THERMAL BARRIER KIT",25901512,3455,null,465,402,576,449,628]
[]
[null,"ACCESSORIES"]
[null,"CONTACK PUCKS"]
[null,"Contact Puck for TSP Single Rigid Sensor with internal sensor"]
[null,"CONTACT PUCK 0",35900031,682,null,92,79,114,89,124]
[null,"Overall dimension ø 30 mm x 8 mm, Stainless Steel AISI 316 , Hole dimension ø 1.3 mm, ø 1.6 mm, ø1.9 mm and ø2.1 mm"]
[null,"MULTI CONTACT PUCK FOR RTD",35900073,889,null,120,103,148,115,162]
[null,"PROTECTIVE SLEEVE AND HOLDERS"]
[null,"Protective sleeve for TSP Logger",25900002,770,null,104,90,128,100,140]
[null,"Protective sleeve for Mini logger",25900077,718,null,97,83,120,93,131]
[null,"Protective sleeve for Micro Logger",25900078,718,null,97,83,120,93,131]
[null,"Protective holder for Pro/Basic loggers",25900089,847,null,114,98,141,110,154]
[null,"Protective holder for Compact loggers",25900090,847,null,114,98,141,110,154]
[null,"LOGGER FIX - Peek holder for TSP Loggers",35900003,838,null,113,97,140,109,152]
[null,"FIX PRO CASE - Silicone Logger Holder, 1 pcs.",35900000,586,null,79,68,98,76,107]
[null,"FIX PRO CASE - Silicone Logger Holder, Set of 25 pcs.",35900001,11759,null,1583,1367,1960,1527,2138]
[null,"SEALENT"]
[null,"Sealant for logger, 10 ml",35900063,123,null,17,14,21,16,22]
[null,"O-RINGS"]
[null,"O-ring for TSP Logger, set of 10 pcs.",35900007,232,null,31,27,39,30,42]
[null,"O-ring for TSP Sensor, outer, set of 20 pcs.",35900008,221,null,30,26,37,29,40]
[null,"O-ring for TSP Sensor, Teflon, set of 2 - for mounting only at Ellab",35900018,276,null,37,32,46,36,50]
[null,"O-ring for TSP Sensor, inner, set of 10 pcs.",35900009,139,null,19,16,23,18,25]
[null,"O-ring for TSP Mini Logger, set of 10 pcs.",35900010,139,null,19,16,23,18,25]
[null,"O-ring for TSP Micro 1st gen., set of 10 pcs.",35900011,139,null,19,16,23,18,25]
[null,"O-ring for TSP Micro 2nd gen., set of 10 pcs.",35900022,184,null,25,21,31,24,33]
[null,"O-ring for TSP Compact, set of 10 pcs.",35900019,139,null,19,16,23,18,25]
[null,"O-ring for TS Frigo, set of 10 pcs.",35900021,139,null,19,16,23,18,25]
[null,"Black O-ring/rubber washer for TSP rigid sensors with thread, GEJ-C packing gland, SSA probes and stainless steel space bar, 10 pcs"]
[null,"GEJ37007U RUBBER WASHER",25810022,102,null,14,12,17,13,19]
[null,"LOGGER ID RINGS"]
[null,"Set of ID engraved stainless steel top rings for TSP loggers"]
[null,"LOGGER ID RING 1-12",35105999,3768,null,507,438,628,489,685]
[null,"LOGGER ID RING 13-24",35105998,3768,null,507,438,628,489,685]
[null,"LOGGER ID RING 25-36",35105997,3768,null,507,438,628,489,685]
[null,"LOGGER ID RING 37-48 ",35105996,3768,null,507,438,628,489,685]
[null,"LOGGER ID RING 49-60",35105995,3768,null,507,438,628,489,685]
[null,"LOGGER ID RING 61-73",35105994,3768,null,507,438,628,489,685]
[null,"LOGGER ID RING 74-85",35105993,3768,null,507,438,628,489,685]
[null,"LOGGER ID RING 86-97",35105992,3768,null,507,438,628,489,685]
[null,"LOGGER ID RING 98-109",35105991,3768,null,507,438,628,489,685]
[null,"LOGGER ID RING 110-121",35105990,3768,null,507,438,628,489,685]
[null,"LOGGER ID RING 122-134",35105989,3768,null,507,438,628,489,685]
[]
[null,"PACKING GLANDS"]
[null,"PACKING GLANDS FOR INTERNAL MOUNTING"]
[]
[null,"TSK08000Q054 PEEK - Internal fixture for TS Pro Loggers, peek",25901074,1313,null,177,153,219,171,239]
[null,"TSJ08000Q054 - Internal fixture for TS Pro loggers, stainless steel",25901082,1313,null,177,153,219,171,239]
[null,"TSJ08000Q072 - Internal fixture for Compact Loggers, stainless steel",25901099,1313,null,177,153,219,171,239]
[null,"TSK MINI 2G PEEK - Internal fixture for Mini Logger 2. Gen, peek",35411082,1169,null,157,136,195,152,213]
[null,"TSJ MINI 2G STEEL - Internal fixture for Mini Logger 2. Gen, steel",35411080,1169,null,157,136,195,152,213]
[null,"TSJ MICRO PRS/TMP 2G - Internal fixture for Micro PRS/TMP logger 2nd Gen.",35401090,1499,null,202,174,250,195,273]
[null,"Distance Piece for both Pro, Mini & Micro Internal fixture, for different measuring depths"]
[null,"TKK10PROL0XX STAKE f. FIXTURE","354500XX",297,null,40,35,50,39,54]
[null,"INTERNAL FIXTURE"]
[null,"(sample of the packaging necessary)"]
[null,"TBJ BOTTLE/CAN - Internal fixture for Bottle & Can",35000109,1716,null,231,200,286,223,312]
[null,"TPJ FLAT POUCHES - Internal fixture for flat pouches",35000113,1493,null,201,174,249,194,271]
[null,"PACKING GLANDS WITH STAINLESS STEEL TUBE IN SPECIAL LENGTHS"]
[null,"Please replace XXX with length (min. 27 mm)"]
[null,"GKJ21009CXXX PACKING GLAND","35901XXX",782,null,105,91,130,102,142]
[null,"PACKING GLANDS FOR AMPOULES AND VIALS"]
[null,"Packing gland for ampoules\nYY: please specify ampoule diameter (11, 15, 22)\nXX: please specify size of ampoule (1, 2, 3, 5, 10, 20, 25, 30 ml)"]
[null,"GNK210YYC0XX PACKING GLAND","2590002X",1442,null,194,168,240,187,262]
[null,"Silicone rubber packing, 10 pcs.",25810080,444,null,60,52,74,58,81]
[null,"GLJ25050C005 PACKING GLAND for plastic vials",25810708,1135,null,153,132,189,147,206]
[null,"LYOSTOPPERS FOR TSP LOGGERS"]
[null,"Diameter: 13 or 20mm"]
[null,"LYO 13 mm for ø1,2mm sensor",35903200,1125,null,151,131,188,146,205]
[null,"LYO 20 mm for ø1,2mm sensor",35903201,1125,null,151,131,188,146,205]
[null,"LYO 13 mm for ø1,8 flex sensor",35903204,1125,null,151,131,188,146,205]
[null,"LYO 20 mm for ø1,8 flex sensor",35903205,1125,null,151,131,188,146,205]
[null,"PACKING GLANDS FOR IV-BAGS, PLAST BARRELS"]
[]
[null,"GLK20050C005 - Packing Gland for plast ampoules, syringe barrels, with cone in PEEK",25810707,1135,null,153,132,189,147,206]
[null,"SPACE BARS IN SPECIAL LENGTHS"]
[null,"Special space bar length from 10 mm to 115 mm."]
[null,"Please replace XXX with length in mm."]
[null,"GKJ31008JXXX - Space bar in stainless steel.","25903XXX",378,null,51,44,63,49,69]
[null,"Please replace XXX with length in mm. (min. 10mm length)"]
[null,"GKK31008KXXX - Space bar in PEEK.","259040XX",325,null,44,38,54,42,59]
[null,"SPACE BARS IN STANDARD LENGTHS"]
[]
[null,"GKJ31008J010 - 10 mm space bar in stainless steel",25903010,259,null,35,30,43,34,47]
[null,"GKJ31008J015 - 15 mm space bar in stainless steel",25903015,293,null,39,34,49,38,53]
[null,"GKK31008K010 - 10 mm space bar in PEEK",25904010,213,null,29,25,36,28,39]
[null,"GKK31008K015 - 15 mm space bar in PEEK",25904015,213,null,29,25,36,28,39]
[null,"GKK31008K020 - 20 mm space bar in PEEK",25904020,213,null,29,25,36,28,39]
[null,"GKK31008K025 - 25 mm space bar in PEEK",25904025,213,null,29,25,36,28,39]
[null,"GKK31008K030 - 30 mm space bar in PEEK",25904030,213,null,29,25,36,28,39]
[null,"GKK31008K035 - 35 mm space bar in PEEK",25904035,213,null,29,25,36,28,39]
[null,"GKK31008K040 - 40 mm space bar in PEEK",25904040,213,null,29,25,36,28,39]
[null,"GKK31008K045 - 45 mm space bar in PEEK",25904045,213,null,29,25,36,28,39]
[null,"GKK31008K050 - 50 mm space bar in PEEK",25904050,213,null,29,25,36,28,39]
[null,"Rubber washers for space bar"]
[null,"GKK49006U - Rubber Washer White, PEEK, 10 pcs.",25900057,102,null,14,12,17,13,19]
[null,"GKJ37007U - Rubber Washer Red, PEEK, 10 pcs",25900056,102,null,14,12,17,13,19]
[null,"DISTANCE PIECES"]
[null,"Please replace XXX with length. From 10 - 150 mm in steps of 5 mm."]
[null,"GEM21008KXXX - Distance piece","258102XX",331,null,45,38,55,43,60]
[null,"Distance piece for use with GKJ.\nPlease replace XXX with length. From 10 - 150 mm in steps of 5 mm."]
[null,"GEM31008KXXX - Distance piece","259011XX",331,null,45,38,55,43,60]
[null,"RUBBER PACKINGS FOR MOUNTING IN AUTOCLAVES - SKY"]
[null,"for autoclave packing glands, type GRJ, GQJ and GSJ"]
[null,"GQJ60024S001 - Rubber packing ½\" with 1 hole for Sky Antenna",25800088,573,null,77,67,96,74,104]
[null,"GRJ60027S001 - Rubber packing 3/4\" with 1 hole for Sky Antenna",25800090,573,null,77,67,96,74,104]
[]
[null,"TOOLS"]
[null,"CUTTING TOOLS AND SPANNERS"]
[null,"TC35 - Bending tool for SemiFlex",25000104,497,null,67,58,83,65,90]
[null,"TC 25 - Cutting tool for HUJ and GUJ",25000009,398,null,54,46,66,52,72]
[null,"TC 26 - ELLAB Spanner for HUJ and GUJ",25000014,1365,null,184,159,228,177,248]
[null,"TC 41 - Pre-perforator for TC 40S below",25000010,679,null,91,79,113,88,123]
[null,"TC 40S - Cutting tool for metal containers",25000044,2179,null,293,253,363,283,396]
[null,"TC 42 - Cutting tool for plast containers, ø8 mm",25000012,278,null,37,32,46,36,51]
[null,"TC 89 - Can punch for all kinds of containers",25000018,7243,null,975,842,1207,941,1317]
[null,"SENSOR REMOVAL TOOL"]
[null,"Sensor Removal Tool",25000027,1711,null,230,199,285,222,311]
[null,"FRIGO UX SKY REMOVAL TOOL, 30 mm",25000107,1696,null,228,197,283,220,308]
[]
[null,"SUITCASES & FLIGHTCASES"]
[null,"SMALL SUITCASES"]
[null,"Dimensions: 34 x 27.5 x 8.3 cm"]
[null,"Suitcase for TSP 22 loggers and sensors (small)",21203061,2262,null,304,263,377,294,411]
[null,"Suitcase for loggers etc.",21203010,985,null,133,115,164,128,179]
[null,"LARGE SUITCASES"]
[null,"Dimensions: 45 x 36 x 10.6 cm"]
[null,"Standard suitcase TS PRO Equipment and 22 Loggers",21203050,3151,null,424,366,525,409,573]
[null,"Suitcase for TSP SKY access point and 22 loggers & SKY module",21203052,3151,null,424,366,525,409,573]
[null,"Suitcase for TS Pro 44 loggers and sensors",21203051,3634,null,489,423,606,472,661]
[null,"SUITCASE FRIGO UX SKY",21203001,3151,null,424,366,525,409,573]
[null,"SUITCASE FRIGO UX SKY + Readerstation",21203002,3151,null,424,366,525,409,573]
[null,"FLIGHTCASES"]
[null,"For Demo Kit"]
[null,"Flight case EVPP/TSP/LYO/TVP",21206003,13614,null,1832,1583,2269,1768,2475]
[null,"Flightcase EVPP/TSP/LYO/TVP - Additional Layer",21206004,653,null,88,76,109,85,119]
[]
[]
[null,"* Prices for Optional Additional Software Drivers, Software Upgrades and Extra Software Licenses can be found under the ValSuite-tab"]

{"sheet":"TrackSense LyoPro","index":1,"n_rows":73,"n_cols":10,"rows_kept":73,"cut":false,"hidden":false,"merged":[[0,8,1,9],[72,1,72,9],[71,1,71,9],[8,1,8,9],[29,1,29,9],[43,1,43,9],[69,1,69,9],[70,1,70,9],[57,1,57,9]]}
[null,"Ellab Validation Solutions",null,null,null,null,null,null,{"$error":"#VALUE!"}]
[null,"Parts List: TrackSense LyoPro"]
[null,"Validation Pricing Ver. 03 - July 2026"]
[null,"15 July 2026 to 31 December 2026"]
[null,null,null,null,null,"DKK/€","DKK/£","DKK/$","DKK/CHF","DKK/Japan US"]
[null,null,null,null,null,7.43,8.6,6,7.7,5.5]
[null,"Description","Ellab Ordering\nCode","RRP DKK","Discount","RRP €","RRP £","RRP US$","RRP CHF","Japan US$"]
[null,"TRACKSENSE LYOPRO READER STATION AND ACCESS POINT"]
[]
[null,"TrackSense® LyoPro Reader Station incl. 1 ValSuite Pro",31200000,104046,null,14003,12098,17341,13512,18917]
[null,"TrackSense® LyoPro Access Point",31206000,41621,null,5602,4840,6937,5405,7567]
[null,"TS LyoPro Dual Internal Antenna",31206010,12694,null,1708,1476,2116,1649,2308]
[]
[null,"TRACKSENSE LYOPRO LOGGER"]
[null,"Logger incl. sensor and 1 battery\nStandard Calibration Points: -60, -30, 0, 30, 60 C"]
[null,"TS LyoPro Logger with 30 cm TC Sensor AWG 30",31201000,27750,null,3735,3227,4625,3604,5045]
[null,"TS LyoPro Logger with 50 cm TC Sensor AWG 30",31201050,27750,null,3735,3227,4625,3604,5045]
[]
[null,"CONSUMABLES"]
[null,"BATTERIES"]
[null,"High Performance Battery for LyoPro Loggers\nNote: Dangerous Goods fee might apply when shipping batteries"]
[null,"TSL BATTERY with Activator",31200050,1037,null,140,121,173,135,189]
[null,"TSL BATTERY without Activator",31200051,777,null,105,90,130,101,141]
[null,"TC SENSOR"]
[null,"TS PRO Thermocouple, 30 cm",35123523,444,null,60,52,74,58,81]
[null,"O-RING"]
[null,"O-RING FOR LYOPRO, 1 pc.",31209111,21,null,3,2,4,3,4]
[]
[null,"TRACKSENSE LYOPRO ACCESSORIES LOGGER NEST"]
[null,"Accessories for ISO Standard Vials"]
[null,"Logger Nest for vial type 2R",31203021,606,null,82,70,101,79,110]
[null,"Logger Nest for vial type 4R",31203041,625,null,84,73,104,81,114]
[null,"Logger Nest for vial type 6R",31203061,738,null,99,86,123,96,134]
[null,"Logger Nest for vial type 8R",31203081,704,null,95,82,117,91,128]
[null,"Logger Nest for vial type 10R",31203101,782,null,105,91,130,102,142]
[null,"Logger Nest for vial type 15R",31203151,1098,null,148,128,183,143,200]
[null,"Logger Nest for vial type 20R",31203201,1010,null,136,117,168,131,184]
[null,"Logger Nest for vial type 25R",31203251,1405,null,189,163,234,182,255]
[null,"Logger Nest for vial type 30R",31203301,1836,null,247,213,306,238,334]
[null,"Logger Nest for vial type 50R",31203501,1870,null,252,217,312,243,340]
[null,"Logger Nest for vial type 100R",31203001,1919,null,258,223,320,249,349]
[]
[null,"TRACKSENSE LYOPRO STOPPER CLIP"]
[null,"Accessories for ISO Standard Vials"]
[null,"StopperClip 2R",31208023,2237,null,301,260,373,291,407]
[null,"StopperClip 4R",31208043,2237,null,301,260,373,291,407]
[null,"StopperClip 6R",31208063,2237,null,301,260,373,291,407]
[null,"StopperClip 8R",31208083,2237,null,301,260,373,291,407]
[null,"StopperClip 10R",31208103,2237,null,301,260,373,291,407]
[null,"StopperClip 15R",31208153,2403,null,323,279,401,312,437]
[null,"StopperClip 20R",31208203,2403,null,323,279,401,312,437]
[null,"StopperClip 25R",31208253,2403,null,323,279,401,312,437]
[null,"StopperClip 30R",31208303,2403,null,323,279,401,312,437]
[null,"StopperClip 50R",31208503,2566,null,345,298,428,333,467]
[null,"StopperClip 100R",31208003,2566,null,345,298,428,333,467]
[]
[null,"TRACKSENSE LYOPUCK"]
[]
[null,"LyoPuck for shelf measurement",31200080,1284,null,173,149,214,167,233]
[]
[null,"SUITCASES"]
[null,"SMALL SUITCASES"]
[null,"Dimensions: 34 x 27.5 x 8.3 cm"]
[null,"Suitcase for 52 LyoPro Loggers",31209100,3268,null,440,380,545,424,594]
[null,"LARGE SUITCASES"]
[null,"Dimensions: 45 x 36 x 10.6 cm"]
[null,"Suitcase for 80 LyoPro Loggers",31209101,3872,null,521,450,645,503,704]
[]
[]
[null,"* TraceSense LyoPro Connecting Clip, Buffer Clip and LyoStoppers for ISO vials 2R to 100R can still be purchased"]
[null,"* TraceSense LyoPro Accessories Vial Adapt Packages, which contains Logger Nest, Connecting Clip, Buffer Clip and LyoStopper can still be purchased"]
[null,"* Price for ValSuite OPC can be found under the ValSuite-tab "]
[null,"* Price for additional TC Sensors, please see TrackSense Pro Low Temperature Sensors"]

{"sheet":"TrackSense Lab","index":2,"n_rows":27,"n_cols":10,"rows_kept":27,"cut":false,"hidden":false,"merged":[[9,1,9,9],[14,1,14,9],[0,8,1,9]]}
[null,"Ellab Validation Solutions",null,null,null,null,null,null,{"$error":"#VALUE!"}]
[null,"Parts List: TrackSense Lab"]
[null,"Validation Pricing Ver. 03 - July 2026"]
[null,"15 July 2026 to 31 December 2026"]
[null,null,null,null,null,"DKK/€","DKK/£","DKK/$","DKK/CHF","DKK/Japan US"]
[null,null,null,null,null,7.43,8.6,6,7.7,5.5]
[null,"Description","Ellab Ordering\nCode","RRP DKK","Discount","RRP €","RRP £","RRP US$","RRP CHF","Japan US$"]
[null,"DATA LOGGERS"]
[null,"TEMPERATURE"]
[null,"Logger incl. sensor and 1 battery\nQuantity discount: 5% at more than 10 units, 10% at more than 25 units, 15% at more than 50 units"]
[null,"TrackSense Lab Logger, -30 to +100°C, with alarm indicator, with internal sensor",36303000,9283,null,1249,1079,1547,1206,1688]
[null,"TrackSense Lab Logger, -30 to +100°C, with alarm indicator, with 35 mm sensor",36303035,9750,null,1312,1134,1625,1266,1773]
[null,"TrackSense Lab Quad Logger with 4 channels 1,8 mm Teflon Sensors. Length 50 cm. -30 to +100°C",36303200,29403,null,3957,3419,4901,3819,5346]
[null,"RELATIVE HUMIDITY"]
[null,"Logger incl. sensor and 1 battery.\nRequires ValSuite 5.2.0.10 or later. \nQuantity discount: 5% at more than 10 units, 10% at more than 25 units, 15% at more than 50 units"]
[null,"TrackSense Lab Data Logger - Relative Humidity & Temperature Sensor (ex LED)",36303100,14273,null,1921,1660,2379,1854,2595]
[null,"SKY MODULE"]
[]
[null,"SKY MODULE LAB 3G",31190520,4239,null,571,493,707,551,771]
[]
[null,"CONSUMABLES"]
[null,"BATTERIES"]
[null,"High Performance Battery for Pro, Basic, Compact and Lab Loggers\nNote: Dangerous Goods fee might apply when shipping batteries"]
[null,"TSP BATTERY with Activator",35900050,1037,null,140,121,173,135,189]
[null,"TSP BATTERY without Activator",35900051,777,null,105,90,130,101,141]
[null,"O-RING"]
[null,"O-ring for TSP & TS Mini Logger, set of 10 pcs.",35900010,139,null,19,16,23,18,25]

{"sheet":"SteriSense","index":3,"n_rows":28,"n_cols":10,"rows_kept":28,"cut":false,"hidden":false,"merged":[[8,1,8,9],[12,1,12,2],[26,1,26,2],[22,1,22,2],[0,8,1,9]]}
[null,"Ellab Validation Solutions",null,null,null,null,null,null,{"$error":"#VALUE!"}]
[null,"Parts List: SteriSense"]
[null,"Validation Pricing Ver. 03 - July 2026"]
[null,"15 July 2026 to 31 December 2026"]
[null,null,null,null,null,"DKK/€","DKK/£","DKK/$","DKK/CHF","DKK/Japan US"]
[null,null,null,null,null,7.43,8.6,6,7.7,5.5]
[null,"Description","Ellab Ordering\nCode","RRP DKK","Discount","RRP €","RRP £","RRP US$","RRP CHF","Japan US$"]
[null,"STERISENSE READER STATION AND SOFTWARE"]
[null,"Including: USB cable, Carrying Case and license for 1 computer "]
[null,"STERISENSE PRO SINGLE READER STATION",32189001,30695,null,4131,3569,5116,3986,5581]
[]
[null,"STERISENSE UNITS"]
[null,"Calibration points: 25°C, 70°C, 140°C / 50, 1000, 3000 mBar\nOnly for 134°C and Medical customers.\nRequires SteriSense Software or ValSuite Medical/ Plus version 5.3 or later."]
[null,"SteriSense Unit (Logger, Battery, Sensor, Protective Adaptor & PCD)",31193100,27500,null,3701,3198,4583,3571,5000]
[null,"Process Challenge Device (PCD)",35000500,2238,null,301,260,373,291,407]
[]
[null,"CONSUMABLES"]
[null,"BATTERIES"]
[null,"Note: Dangerous Goods fee might apply when shipping batteries"]
[null,"TSP Battery 150L with Activator. Only for Compact Ultra X and TS Pro XL logger",35900055,1037,null,140,121,173,135,189]
[]
[null,"EXTRA SOFTWARE LICENCES"]
[null,"When ordering, please state full legal customer name and present serial number or license key of software"]
[null,"Extra ValSuite SteriSense License, 10 pcs.",35550091,30678,null,4129,3567,5113,3984,5578]
[]
[null,"CALIBRATION"]
[]
[null,"Calibration of SteriSense Unit - max 1000 test cycles",9000140,6551,null,882,762,1092,851,1191]

{"sheet":"E-Val Pro","index":4,"n_rows":169,"n_cols":10,"rows_kept":169,"cut":false,"hidden":false,"merged":[[0,8,1,9],[117,1,117,4],[155,1,155,4],[113,1,113,9],[122,1,122,4],[12,1,12,9],[168,1,168,9],[110,1,110,4],[99,1,99,9],[104,1,104,9],[8,1,8,9],[32,1,32,9],[41,1,41,9],[46,1,46,9],[49,1,49,9],[51,1,51,9],[53,1,53,9],[76,1,76,9],[90,1,90,9],[47,1,47,2]]}
[null,"Ellab Validation Solutions",null,null,null,null,null,null,{"$error":"#VALUE!"}]
[null,"Parts List: E-Val Pro"]
[null,"Validation Pricing Ver. 03 - July 2026"]
[null,"15 July 2026 to 31 December 2026"]
[null,null,null,null,null,"DKK/€","DKK/£","DKK/$","DKK/CHF","DKK/Japan US"]
[null,null,null,null,null,7.43,8.6,6,7.7,5.5]
[null,"Description","Ellab Ordering\nCode","RRP DKK","Discount","RRP €","RRP £","RRP US$","RRP CHF","Japan US$"]
[null,"E-VAL PRO VALIDATION SYSTEM"]
[null,"System including:\n- E-VAL PRO PLUS Master, 10” touch color display, 0-52 ch (without sensor arrays), 12 hours rechargeable battery, including ValSuite Pro software with license for 2 computers. \n- The software is validated, 21 CFR part 11 compliant and developed according to GAMP.\n- Power Cable and Carrying Case included."]
[null,"E-VAL PRO PLUS",21602020,158812,null,21374,18467,26469,20625,28875]
[]
[null,"E-VAL PRO VALIDATION SYSTEM WITHOUT SOFTWARE"]
[null,"System including:\n- E-VAL PRO PLUS Master, 10” touch color display, 0-52 ch (without sensor arrays), 12 hours rechargeable battery. \n- Power Cable and Carrying Case included.\n- For Existing Customers Only. "]
[null,"E-Val Pro Plus wired validation system without software",21602021,120223,null,16181,13979,20037,15613,21859]
[]
[null,"E-VAL PRO SENSOR ARRAYS"]
[null,"Including Calibration"]
[null,"E-Val Pro 12 channel Galvanic Insulated TC sensor array",21600013,30931,null,4163,3597,5155,4017,5624]
[null,"E-Val Pro 4 channel Galvanic Insulated TC sensor array",21600014,11786,null,1586,1370,1964,1531,2143]
[null,"E-VAL Pro 12 channel TC sensor array",21600010,22098,null,2974,2570,3683,2870,4018]
[null,"E-VAL Pro 4 channel Multipurpose 4-20 mA/0-10V sensor array",21600011,7882,null,1061,917,1314,1024,1433]
[]
[null,"SENSOR PLUGS WITH SCREW TERMINALS"]
[]
[null,"E-VAL Pro Sensor Plug with screw terminals (TC - thermocouples type T)",25106000,1213,null,163,141,202,158,221]
[null,"E-VAL Pro Sensor Plug with screw terminals (TC), set of 50 pcs.",25106002,51062,null,6872,5937,8510,6631,9284]
[null,"E-VAL Pro Sensor Plug with screw terminals , 4-20 mA",25106003,2031,null,273,236,339,264,369]
[null,"E-VAL Pro Sensor Plug with screw terminals, 0-10V",25106004,2031,null,273,236,339,264,369]
[null,"E-VAL Pro Sensor Plug Digital Input",25106005,1732,null,233,201,289,225,315]
[null,"E-Val Pro Sensor Plug Poly with screw terminals for thermocouples type K,J,N",25106007,1213,null,163,141,202,158,221]
[]
[null,"PRESSURE MEASUREMENT WITH SENSOR INTERFACE"]
[null,"The interface has an operating temperature of -40 to +125°C (cable limited to -40° to 70°C) a pressure range of 0.001 mBar to 10 Bar and a 5 m cable"]
[null,"EVP sensor interface",25106008,5928,null,798,689,988,770,1078]
[null,"TS PRO Pressure Sensor, 4 bar, SKY",35127024,13417,null,1806,1560,2236,1742,2439]
[null,"EVP sensor interface adaptor 1/2\"",21412011,922,null,124,107,154,120,168]
[null,"EVP sensor interface adaptor 3/4\"",21412012,922,null,124,107,154,120,168]
[null,"1½\" Flange Adaptor (DN40) with ½\" internal thread",21412007,2373,null,319,276,396,308,431]
[null,"1½\" Flange Adaptor (DN40) with 3/4\" internal thread",21412004,2373,null,319,276,396,308,431]
[]
[null,"SPARES FOR PAJDIGITALC030 PRESSURE KIT"]
[]
[null,"Pressure connection kit for containers",21412005,5538,null,745,644,923,719,1007]
[null,"Internal capillary tube",25520027,1532,null,206,178,255,199,279]
[]
[null,"STRUCTURE OF TYPE DESIGNATION FOR PROBES WITH SMART USB CONNECTOR"]
[null,"As standard, probes are NOT calibrated\nType designation example:\nSSA = Description of electrode built-up. 12100=Electrode dimension in mm (1,2 dia x 100). P = Plug type (Smart USB connector)\n700 = Length of cable. Up to 9 m in cm and more than 10 m in meters. Available in full meters only.\nTS = Type of cable. TS = Silicone cable. TF = PTFE cable."]
[null,"ADDITIONAL PRICE FOR SPECIAL CABLE LENGTH FOR PROBES\nFrom 7 m, per meter:  When ordering special length, please remember to specify the type designation."]
[null,"SSA12100PXXXTS","251060XX",133,null,18,15,22,17,24]
[null,"ADDITIONAL PRICE FOR SPECIAL ELECTRODE LENGTH FOR PROBES\nWhen ordering special length, please remember to specify the type designation. Standard lenghts of electrode are: 50, 80, 100 and 115 mm"]
[null,"SSA12XXXP700TS","25106XXX",293,null,39,34,49,38,53]
[null,"ADDITIONAL PRICE FOR STANDARD REINFORCEMENTS"]
[null,"SSA12100X700TS-XX","251XXXXX",523,null,70,61,87,68,95]
[null,"ADDITIONAL PRICE FOR NON-STANDARD REINFORCEMENT -33 (1500 mm spring) AND REINFORCEMENT -20 (Transparent Silicone Hose in full cable lenght)"]
[null,"SSA12100X700TS-33 AND -20","25XXXXXX",1635,null,220,190,273,212,297]
[]
[null,"THERMOCOUPLE PROBES WITH SMART USB CONNECTOR"]
[null,"THERMOCOUPLE PROBES WITH SMART USB CONNECTOR"]
[null,"Length 7 meter\nMeasuring point 4 mm from tip\nAs standard, probes are NOT calibrated"]
[null,"SSA Probe, Needle 1,2 dia x 50 mm, rounded point, 7 meter",25106013,2383,null,321,277,397,309,433]
[null,"SSA Probe, Needle 1,2 dia x 80 mm, rounded point, 7 meter",25106014,2383,null,321,277,397,309,433]
[null,"SSA Probe, Needle 1,2 dia x 100 mm, rounded point, 7 meter",25106015,2383,null,321,277,397,309,433]
[null,"SSA Probe, Needle 1,2 dia x 115 mm, rounded point, 7 meter",25106016,2383,null,321,277,397,309,433]
[null,"STC THERMOCOUPLE PROBES WITH SMART USB CONNECTOR"]
[null,"Moist and heat resistant probe.\nLength 7 meter\nAs standard, probes are NOT calibrated"]
[null,"STC - Flexible PTFE probe ø3,2 mm x 7 meter cable, up to +200 °C",25106023,1463,null,197,170,244,190,266]
[null,"STC - Flexible PTFE probe ø2,2 mm x 7 meter cable, up to +200 °C",25106024,1487,null,200,173,248,193,270]
[null,"STC - Flexible PTFE probe ø3,2 mm x 7 meter cable, without plug, up to +200°C",25101559,1102,null,148,128,184,143,200]
[null,"HIGH TEMPERATURE PROBES WITH SMART USB CONNECTOR"]
[null,"For hot air measurements. \nLength 7 meter.\nAs standard, probes are NOT calibrated\nShort term: Max 30 minutes at the specified temperature."]
[null,"STC - Flexible Kapton Probe, 7 meter, up to +260°C (+350°C short term), 3 strand cable",25106011,1584,null,213,184,264,206,288]
[null,"STC - Flexible Kapton Probe, 7 meter, up to +260°C (+350°C short term), 7 strand cable",25106012,1711,null,230,199,285,222,311]
[null,"SSU - High Temperature Probe, metal sheathed, up to +300°C (+400°C short term)",25106018,2666,null,359,310,444,346,485]
[]
[null,"FEED THROUGH SYSTEM FOR STC PROBES"]
[null,"FEED THROUGHS"]
[]
[null,"Feed Through 1.5\" Flange up to 20 TCs incl. silicone disc set",21412021,15368,null,2068,1787,2561,1996,2794]
[null,"Feed Through 1.5\" Flange up to 50 TCs incl. silicone disc set",21412022,21668,null,2916,2520,3611,2814,3940]
[null,"ACCESSORIES"]
[null,"Tri Clamp 1½ \"",21412024,555,null,75,65,93,72,101]
[null,"Gasket for Tri Clamp 1½\"",21412025,97,null,13,11,16,13,18]
[null,"Silicone disc set for FT 20, set of 3 pcs.",21412031,1160,null,156,135,193,151,211]
[null,"T-Piece adaptor 1½\"  with Digital Pressure sensor adaptor, 3 pcs TriClamps, Gaskets, and 1 lid",21412033,18745,null,2523,2180,3124,2434,3408]
[null,"T-Piece adaptor 1 ½\"",21412023,14029,null,1888,1631,2338,1822,2551]
[null,"Lid for T-Piece",21412026,414,null,56,48,69,54,75]
[null,"1½\" Flange Adaptor (DN40) with ½\" internal thread",21412007,2373,null,319,276,396,308,431]
[]
[null,"RUBBER PACKINGS FOR AUTOCLAVE PACKING GLANDS"]
[null,"RUBBER PACKINGS FOR AUTOCLAVE PACKING GLANDS - FOR SILICONE CABLES"]
[null,"Hole diameter: 4mm"]
[null,"GQJ40024S004 - Rubber Packing with 4 holes, ½\"",25800003,147,null,20,17,25,19,27]
[null,"GRJ40027S004 - Rubber Packing with 4 holes, ¾\"",25800007,147,null,20,17,25,19,27]
[null,"GRJ40027S006 - Rubber packing with 6 holes, ¾\"",25800008,186,null,25,22,31,24,34]
[null,"GRJ40027S008 - Rubber Packing with 8 holes, ¾\"",25800018,221,null,30,26,37,29,40]
[null,"GSJ40036S012 - Rubber Packing with 12 holes, 1\"",25800025,410,null,55,48,68,53,75]
[null,"GSJ40036S016 - Rubber packing with 16 holes, 1\"",25800057,410,null,55,48,68,53,75]
[null,"Channel Blocker for rubber packings with ø4 mm holes",25800103,36,null,5,4,6,5,7]
[null,"RUBBER PACKINGS FOR AUTOCLAVE PACKING GLANDS - FOR PTFE CABLES"]
[null,"Hole diameter: 2mm"]
[null,"GQJ20024S008 - Rubber Packing with 8 holes, ½\"",25800064,573,null,77,67,96,74,104]
[null,"GRJ20027S016 - Rubber Packing with 16 holes, ¾\"",25800065,573,null,77,67,96,74,104]
[null,"Channel Blocker for rubber packings with ø2 mm holes",25800104,36,null,5,4,6,5,7]
[null,"RUBBER PACKINGS FOR AUTOCLAVE PACKING GLANDS - SPECIAL "]
[]
[null,"GQJ00024S - Rubber packing without holes, ½\"",25800004,70,null,9,8,12,9,13]
[null,"GRJ00027S - Rubber packing without holes, ¾\"",25800009,70,null,9,8,12,9,13]
[]
[null,"ACCESSORIES FOR PROBES"]
[null,"O-RINGS"]
[null,"Black O-ring/rubber washer for TSP rigid sensors with thread, GEJ-C packing gland, SSA probes and stainless steel space bar, 10 pcs"]
[null,"GEJ37007U RUBBER WASHER",25810022,102,null,14,12,17,13,19]
[null,"ID LABELS"]
[null,"Shrink tube ID-labels for STC thermocouples, yellow with black text. Max. temp. +200°C"]
[null,"ID-LABEL 1-16 - Shrink tube ID-labels for STC thermocouples",25105999,561,null,76,65,94,73,102]
[null,"SHRINK TUBE ID-LABELS 1-52 Y/B",25105995,1054,null,142,123,176,137,192]
[null,"CONTACK PUCKS"]
[null,"Overall dimension ø34 mm x 12 mm , Stainless Steel AISI 316L , Hole dimension ø 3.5 mm"]
[null,"CONTACT PUCK FOR STC",35900072,682,null,92,79,114,89,124]
[]
[null,"PACKING GLANDS"]
[null,"PACKING GLANDS FOR DIFFERENT CONTAINERS"]
[null,"Internal fixture for flat pouches  (sample of the packaging necessary)"]
[null,"TPJ FLAT POUCHES - Internal fixture for flat pouches",35000113,1493,null,201,174,249,194,271]
[null,"PACKING GLANDS FOR AMPOULES AND VIALS"]
[null,"Packing gland for ampoules.\nYY: please specify ampoule diameter (11, 15, 22)\nXX: please specify size of ampoule (1, 2, 3, 5, 10, 20, 25, 30 ml)"]
[null,"GNK130YYC0XX Packing Gland","2581000X",1442,null,194,168,240,187,262]
[null,"Silicone rubber packing, 10 pcs.",25810080,444,null,60,52,74,58,81]
[null,"PACKING GLANDS FOR BOTTLES"]
[null,"GVK42C - Packing gland for bottle. Sample of bottle necessary","2590XXXX",5327,null,717,619,888,692,969]
[]
[null,"DISTANCE PIECES"]
[null,"Please replace XXX with length. From 10 - 150 mm in steps of 5 mm."]
[null,"GEM21008KXXX - Distance piece","258102XX",331,null,45,38,55,43,60]
[]
[null,"SPACE BARS"]
[null,"SPACE BARS IN SPECIAL LENGTHS"]
[null,"Special space bar length from 10 mm to 115 mm."]
[null,"Please replace XXX with length in mm."]
[null,"GKJ31008JXXX - Space bar in stainless steel.","25903XXX",378,null,51,44,63,49,69]
[null,"Please replace XXX with length in mm. (min. 10mm length)"]
[null,"GKK31008KXXX - Space bar in PEEK.","259040XX",325,null,44,38,54,42,59]
[null,"SPACE BARS IN STANDARD LENGTHS"]
[]
[null,"GKJ31008J010 - 10 mm space bar in stainless steel",25903010,259,null,35,30,43,34,47]
[null,"GKJ31008J015 - 15 mm space bar in stainless steel",25903015,293,null,39,34,49,38,53]
[null,"GKK31008K010 - 10 mm space bar in PEEK",25904010,213,null,29,25,36,28,39]
[null,"GKK31008K015 - 15 mm space bar in PEEK",25904015,213,null,29,25,36,28,39]
[null,"GKK31008K020 - 20 mm space bar in PEEK",25904020,213,null,29,25,36,28,39]
[null,"GKK31008K025 - 25 mm space bar in PEEK",25904025,213,null,29,25,36,28,39]
[null,"GKK31008K030 - 30 mm space bar in PEEK",25904030,213,null,29,25,36,28,39]
[null,"GKK31008K035 - 35 mm space bar in PEEK",25904035,213,null,29,25,36,28,39]
[null,"GKK31008K040 - 40 mm space bar in PEEK",25904040,213,null,29,25,36,28,39]
[null,"GKK31008K045 - 45 mm space bar in PEEK",25904045,213,null,29,25,36,28,39]
[null,"GKK31008K050 - 50 mm space bar in PEEK",25904050,213,null,29,25,36,28,39]
[null,"Black O-ring/rubber washer for TSP rigid sensors with thread, GEJ-C packing gland, SSA probes and stainless steel space bar, 10 pcs"]
[null,"GEJ37007U RUBBER WASHER",25810022,102,null,14,12,17,13,19]
[]
[null,"SUITCASES & FLIGHTCASES"]
[null,"SMALL SUITCASES"]
[null,"Dimensions: 34 x 27.5 x 8.3 cm"]
[null,"Suitcase for 100 pcs. EVP Screw Terminal USB Plugs (small)",21206002,2283,null,307,265,381,296,415]
[null,"FLIGHTCASES"]
[null,"For Demo Kit"]
[null,"Flight case EVPP/TSP/LYO/TVP",21206003,13614,null,1832,1583,2269,1768,2475]
[null,"Flightcase EVPP/TSP/LYO/TVP - Additional Layer",21206004,653,null,88,76,109,85,119]
[]
[]
[null,"* Prices for Optional Additional Software Drivers, Software Upgrades and Extra Software Licenses can be found under the ValSuite-tab"]

{"sheet":"ValSuite 6","index":5,"n_rows":86,"n_cols":10,"rows_kept":86,"cut":false,"hidden":false,"merged":[[72,1,72,2],[0,8,1,9]]}
[null,"Ellab Validation Solutions",null,null,null,null,null,null,{"$error":"#VALUE!"}]
[null,"Parts List: ValSuite 6"]
[null,"Validation Pricing Ver. 03 - July 2026"]
[null,"15 July 2026 to 31 December 2026"]
[null,null,null,null,null,"DKK/€","DKK/£","DKK/$","DKK/CHF","DKK/Japan US"]
[null,null,null,null,null,7.43,8.6,6,7.7,5.5]
[null,"Description","Ellab Ordering\nCode","RRP DKK","Discount","RRP €","RRP £","RRP US$","RRP CHF","Japan US$"]
[null,"VALSUITE 6 - SOFTWARE UPDATES"]
[null,"All updates include license for 2 Computers.\nOne Master Reader Station can be installed on 2 computers.\nWhen ordering, please inform present serial number or licence key of software."]
[null,"VALSUITE BASIC"]
[null,"VALSUITE 2.X TO VAL 6.X",35550006,16829,null,2265,1957,2805,2186,3060]
[null,"VALSUITE 3.X TO VAL 6.X",35550013,8429,null,1134,980,1405,1095,1533]
[null,"VALSUITE 4.X TO VAL 6.X",35550033,4231,null,569,492,705,549,769]
[null,"VALSUITE 5.X TO VAL 6.X",35550067,2123,null,286,247,354,276,386]
[null,"VALSUITE 6.X TO VAL 6.X",35550056,2123,null,286,247,354,276,386]
[null,"VALSUITE 6.X.X TO 6.X.Y",35550061,0,null,0,0,0,0,0]
[null,"VALSUITE MEDICAL"]
[null,"VALSUITE MEDICAL 4.X TO 6.X",35550038,4231,null,569,492,705,549,769]
[null,"VALSUITE MEDICAL 5.X TO 6.X",35550069,2123,null,286,247,354,276,386]
[null,"VALSUITE MEDICAL 6.X TO 6.Y",35550066,2123,null,286,247,354,276,386]
[null,"VALSUITE PLUS"]
[null,"VALSUITE PLUS 3.X TO 6.X",35550008,31746,null,4273,3691,5291,4123,5772]
[null,"VALSUITE PLUS 4.X TO 6.X",35550034,15877,null,2137,1846,2646,2062,2887]
[null,"VALSUITE PLUS 5.X TO 6.X",35550083,7960,null,1071,926,1327,1034,1447]
[null,"VALSUITE PLUS 6.X TO 6.Y",35550058,3996,null,538,465,666,519,727]
[null,"VALSUITE PLUS 6.X.X TO 6.X.Y.",35550062,0,null,0,0,0,0,0]
[null,"VALSUITE PLUS OEM 3.X TO 6.X",35550055,31746,null,4273,3691,5291,4123,5772]
[null,"VALSUITE PLUS OEM 4.X TO 6.X",35550054,15877,null,2137,1846,2646,2062,2887]
[null,"VALSUITE PLUS OEM 5.X TO 6.X",35550084,7960,null,1071,926,1327,1034,1447]
[null,"VALSUITE PLUS OEM 6.X TO 6.Y",35550060,3996,null,538,465,666,519,727]
[null,"VALSUITE PLUS OEM 6.XX TO 6.XY",35550063,0,null,0,0,0,0,0]
[null,"VALSUITE PRO"]
[null,"VALSUITE PRO 2.X TO 6.X",35550007,63469,null,8542,7380,10578,8243,11540]
[null,"VALSUITE PRO 3.X TO 6.X",35550011,31746,null,4273,3691,5291,4123,5772]
[null,"VALSUITE PRO 4.X TO 6.X",35550035,15877,null,2137,1846,2646,2062,2887]
[null,"VALSUITE PRO 5.X TO 6.X",35550081,7960,null,1071,926,1327,1034,1447]
[null,"VALSUITE PRO 6.X TO 6.Y",35550057,3996,null,538,465,666,519,727]
[null,"VALSUITE PRO 6.XX TO 6.XY",35550064,0,null,0,0,0,0,0]
[null,"VALSUITE PRO OEM 3.X TO 6.X",35550031,31746,null,4273,3691,5291,4123,5772]
[null,"VALSUITE PRO OEM 4.X TO 6.X",35550036,15877,null,2137,1846,2646,2062,2887]
[null,"VALSUITE PRO OEM 5.X TO 6.X",35550082,7960,null,1071,926,1327,1034,1447]
[null,"VALSUITE PRO OEM 6.X TO 6.Y",35550059,3996,null,538,465,666,519,727]
[null,"VALSUITE PRO OEM 6.XX TO 6.XY",35550065,0,null,0,0,0,0,0]
[null,"UPDATE OF EXTRA LICENSES"]
[null,"Update of extra licenses: \n- From ValSuite 2.X to 6.X - Cost of new license(s): 100%\n- From ValSuite 3.X to 6.X - Cost of new license(s): 100%\n- From ValSuite 4.X to 6.X - Cost of new license(s): 60%\n- From ValSuite 5.X to 6.X - Cost of new license(s): 30%\n- From ValSuite 6.X to 6.Y - Cost of new license(s): 15%\n- From ValSuite 6.XX to 6.YY - Cost of new license(s): 0%"]
[null,"LICENSE UPDATE 2 TO 6",35550072,0,null,0,0,0,0,0]
[null,"LICENSE UPDATE 3 TO 6",35550073,0,null,0,0,0,0,0]
[null,"LICENSE UPDATE 4 TO 6",35550074,0,null,0,0,0,0,0]
[null,"LICENSE UPDATE 5 TO 6",35550077,0,null,0,0,0,0,0]
[null,"LICENSE UPDATE 6.X TO 6.Y",35550075,0,null,0,0,0,0,0]
[null,"LICENSE UPDATE 6.XX TO 6.YY",35550076,0,null,0,0,0,0,0]
[]
[null,"ADDITIONAL SOFTWARE DRIVERS - OPTIONAL"]
[null,"VALSUITE OEM"]
[null,"Reference and temperature-standard drivers for ValSuite Pro and Plus Software. \nSold only in connection with ValSuite Plus and Pro System\nIncluding license for 2 Computers"]
[null,"VALSUITE PRO OEM",35550022,21258,null,2861,2472,3543,2761,3865]
[null,"VALSUITE PLUS OEM",35550024,21258,null,2861,2472,3543,2761,3865]
[null,"VALSUITE SCIENTIFIC"]
[null,"ValSuite Scientific Module.\nSold only in connection with ValSuite Basic, Plus and Pro Systems.\nIncluding license for 2 Computers."]
[null,"VALSUITE PRO SCIENTIFIC",35550085,22749,null,3062,2645,3792,2954,4136]
[null,"VALSUITE OPC"]
[null,"Sold only in connection with ValSuite Pro Systems."]
[null,"VALSUITE OPC-UA",35550110,63288,null,8518,7359,10548,8219,11507]
[]
[null,"SOFTWARE UPGRADES"]
[null,"Upgrade prices are for existing version. Therefore an update can also be necessary. \nWhen ordering, please inform present serial number or license key of software. \nAll updates include license for 2 Computers. One Master Reader Station can be installed on 2 Computers."]
[null,"From ValSuite Basic to ValSuite Pro",35550005,47142,null,6345,5482,7857,6122,8571]
[null,"From ValSuite Plus to ValSuite Pro",35550027,25927,null,3490,3015,4321,3367,4714]
[null,"From ValSuite Basic to ValSuite Plus",35550012,24231,null,3261,2818,4039,3147,4406]
[null,"Replacement of lost ValSuite CD's/USB's",35550029,1785,null,240,208,298,232,325]
[]
[null,"EXTRA SOFTWARE LICENSES"]
[null,"When ordering, please state full legal customer name and present serial number or license key of software "]
[null,"Extra Valsuite Pro License, 1 pc.",35550045,8355,null,1124,972,1393,1085,1519]
[null,"Extra Valsuite Pro License, 10 pcs.",35550048,50115,null,6745,5827,8353,6508,9112]
[null,"Extra Valsuite Pro OEM License, 1 pc.",35550046,11557,null,1555,1344,1926,1501,2101]
[null,"Extra Valsuite Pro OEM License, 10 pcs.",35550047,69219,null,9316,8049,11537,8989,12585]
[null,"Extra Valsuite Plus License, 1 pc.",35550041,4995,null,672,581,833,649,908]
[null,"Extra Valsuite Plus License, 10 pcs.",35550044,29810,null,4012,3466,4968,3871,5420]
[null,"Extra Valsuite Plus OEM License, 1 pc.",35550042,8196,null,1103,953,1366,1064,1490]
[null,"Extra Valsuite Plus OEM License, 10 pcs.",35550043,48933,null,6586,5690,8156,6355,8897]
[null,"Extra Valsuite Basic License, 1 pc.",35550037,2315,null,312,269,386,301,421]
[null,"Extra Valsuite Basic License, 10 pcs.",35550040,13789,null,1856,1603,2298,1791,2507]
[null,"Extra Valsuite Scientific License, 1 pc.",35550086,3910,null,526,455,652,508,711]
[null,"Extra Valsuite Scientific License, 10 pcs.",35550087,23412,null,3151,2722,3902,3041,4257]
[null,"Extra ValSuite SteriSense License, 10 pcs.",35550091,30678,null,4129,3567,5113,3984,5578]

{"sheet":"Val EQ - Rental","index":6,"n_rows":127,"n_cols":10,"rows_kept":127,"cut":false,"hidden":false,"merged":[[95,1,95,9],[126,1,126,9],[34,1,34,9],[0,8,1,9],[67,1,67,9],[77,1,77,9],[63,1,63,9],[65,1,65,9],[117,1,117,9],[109,1,109,9],[111,1,111,9],[115,1,115,9],[113,1,113,9],[120,1,120,9],[9,1,9,9],[13,1,13,9],[17,1,17,9],[25,1,25,9],[37,1,37,9],[47,1,47,9],[56,1,56,9],[70,1,70,9],[82,1,82,9],[87,1,87,9],[92,1,92,9],[101,1,101,9],[21,1,21,9],[61,1,61,9],[52,1,52,9]]}
[null,"Ellab Validation Solutions",null,null,null,null,null,null,{"$error":"#VALUE!"}]
[null,"Parts List: Rental"]
[null,"Validation Pricing Ver. 03 - July 2026"]
[null,"15 July 2026 to 31 December 2026"]
[null,null,null,null,null,"DKK/€","DKK/£","DKK/$","DKK/CHF","DKK/Japan US"]
[null,null,null,null,null,7.43,8.6,6,7.7,5.5]
[null,"Description","Ellab Ordering\nCode","RRP DKK","Discount","RRP €","RRP £","RRP US$","RRP CHF","Japan US$"]
[null,"TRACKSENSE PRO"]
[null,"LAPTOP"]
[null,"All prices are per month"]
[null,"1-Month Rental: Validated Laptop",29100000,12807,null,1724,1489,2135,1663,2329]
[null,"1-Month Rental: Non-Validated Laptop with ValSuite Pro License",29100001,6837,null,920,795,1140,888,1243]
[null,"READER STATION"]
[null,"All prices are per month\nIncludes ValSuite Pro Software license for 2 Computers. The software is validated, 21 CFR part 11 compliant"]
[null,"1-Month Rental: TrackSense Pro Multi Reader Station for 4 Pro/Basic/Lab Loggers",29311001,5344,null,719,621,891,694,972]
[null,"1-Month Rental: TrackSense Pro Multi Reader Station for 4 Compact/Frigo Loggers",29310002,5344,null,719,621,891,694,972]
[null,"SKY OPTION"]
[null,"All prices are per month"]
[null,"1-Month Rental: Sky Access Point, RF Receiver, incl. USB and carrying case",29310086,4801,null,646,558,800,624,873]
[null,"1-Month Rental: Sky Module Pro 3G",29310093,939,null,126,109,157,122,171]
[null,"EXPANSION MODULES "]
[null,"All prices are per month\nRequires ValSuite 3.1 or later"]
[null,"1-Month Rental: TrackSense Pro Multi Expansion Module for 4 Pro/Basic/Lab Loggers",29311011,1074,null,145,125,179,139,195]
[null,"1-Month Rental: TrackSense Pro Multi Expansion Module for 4 Compact/Frigo Loggers",29310012,1074,null,145,125,179,139,195]
[null,"LOGGERS WITH SENSORS"]
[null,"All prices are per month.\nAll certificates up to 11 months old.\n1 Battery Included"]
[null,"1-Month Rental: TS Frigo logger -90 to +85 °C, with LED indicator and 35mm rigid sensor",29311900,1347,null,181,157,225,175,245]
[null,"1-Month Rental: TS Frigo Logger -90 to +85 C, 50 cm single SemiFlex sensor, ø1,5mm",29311901,1888,null,254,220,315,245,343]
[null,"1-Month Rental: TS Frigo Logger -90 to +85 C, w/o LED indicator, 30cm single SemiFlex sensor, ø2,0mm",29311902,1574,null,212,183,262,204,286]
[null,"1-Month Rental: Frigo UX Sky Rigid 35mm",29191210,1974,null,266,230,329,256,359]
[null,"1-Month Rental: Frigo UX Sky Rigid 100mm",29191213,1974,null,266,230,329,256,359]
[null,"1-Month Rental: Frigo UX Sky Semiflex 30cm",29191214,2277,null,306,265,380,296,414]
[null,"1-Month Rental: Frigo UX Sky Semiflex 50cm",29191215,2277,null,306,265,380,296,414]
[null,"1-Month Rental: Frigo UX Sky Pressure/Temperature",29191110,2732,null,368,318,455,355,497]
[null,"Relative Humidity Sensor requires ValSuite 5.2.0.10 or later."]
[null,"1-Month Rental: TS Pro Logger 3G Incl. TS Pro RH 5.2",29351219,2133,null,287,248,356,277,388]
[null,"LOGGERS & SENSORS"]
[null,"All prices are per month"]
[null,"1-Month Rental: TS PRO LOGGER 3G, -50 to +150°C, includes new battery",29351230,2154,null,290,250,359,280,392]
[null,"1-Month Rental: TS PRO Single Rigid Sensor, 50 mm, rounded point",29351260,533,null,72,62,89,69,97]
[null,"1-Month Rental: TS PRO Semi Flexible Single Sensor, 50 cm.",29351261,898,null,121,104,150,117,163]
[null,"1-Month Rental: TS PRO TC sensor incl. 30 cm long Thermocouple",29351262,1036,null,139,120,173,135,188]
[null,"1-Month Rental: TS PRO Semi Flexible Double Sensor, 50 cm",29351263,1788,null,241,208,298,232,325]
[null,"1-Month Rental: TS PRO Double Flexible High Temperature Sensor, 50 cm",29351264,1671,null,225,194,279,217,304]
[null,"1-Month Rental: TS PRO Pressure Sensor, 6 bar, SKY",29351265,1540,null,207,179,257,200,280]
[null,"1-Month Rental: TS PRO Bowie Dick Sensor. incl. PCD and protective adaptor",29351267,2351,null,316,273,392,305,427]
[null,"ACCESSORIES FOR RENT"]
[null,"All prices are per month"]
[null,"1-Month Rental: Magnetic Logger Case",29159996,107,null,14,12,18,14,19]
[null,"1-Month Rental: FixPro Case",29159997,107,null,14,12,18,14,19]
[null,"1-Month Rental: Contact Puck for 0mm / Flat Sensor",29159998,107,null,14,12,18,14,19]
[null,"1-Month Rental: Contact Puck for TSP Loggers",29159999,107,null,14,12,18,14,19]
[null,"THERMAL BARRIERS FOR SINGLE OR DOUBLE HIGH TEMPERATURE SENSOR"]
[null,"1-Month Rental: TTB64-2 THERMAL BARRIER DBL., ø64 mm x 150 mm, Max. 50 minutes at +400°C",29151502,1507,null,203,175,251,196,274]
[null,"1-Month Rental: TBF40-2 THERMAL BARRIER, 40x100x153 mm, Max. 40 minutes at +400°C",29151500,1704,null,229,198,284,221,310]
[null,"MANDATORY AS FOUND CALIBRATION AFTER RETURN"]
[null,"Temperature: \"as found\" calibration certificate after return - 3 standard points."]
[null,"1-Month Rental: Mandatory Calibration TMP TSP Single Sensor",29900005,605,null,81,70,101,79,110]
[null,"1-Month Rental: Mandatory Calibration TMP TSP Frigo Single Sensor",29900006,755,null,102,88,126,98,137]
[null,"1-Month Rental: Mandatory Calibration TMP TSP Dual Sensor",29900037,905,null,122,105,151,118,165]
[null,"1-Month Rental: Mandatory Calibration TMP TC Sensor",29900007,1212,null,163,141,202,157,220]
[null,"Pressure: \"as found\" calibration certificate after return - standard points."]
[null,"1-Month Rental: Mandatory Calibration PRS TSP Sensor",29900022,1007,null,136,117,168,131,183]
[null,"CO2: \"as found\" calibration certificate after return - standard points."]
[null,"1-Month Rental: Mandatory Calibration CO2 TSP Sensor",29900067,755,null,102,88,126,98,137]
[null,"Relative Humidity: \"as found\" calibration certificate after return - standard points."]
[null,"1-Month Rental: Mandatory Calibration RH/TMP TSP Sensor",29900024,1007,null,136,117,168,131,183]
[null,"DANAK - ACCREDITED CALIBRATION\nAdditional charge 25%.\nPlease inform customer name for certificate."]
[null,"DANAK TMP - Accredited Calibration Certificate DANAK for Temperature",9000090,0,null,0,0,0,0,0]
[null,"OPTIONAL ACCREDITED PRE-CAL. CERTIFICATE"]
[null,"Please inform full customer name for certificate"]
[null,"Temperature"]
[null,"1-Month Rental: Accredited Pre-Calibration Certificate DANAK - TMP TSP Single Sensor",29900015,755,null,102,88,126,98,137]
[null,"1-Month Rental: Accredited Pre-Calibration Certificate DANAK - TMP TSP Frigo Sensor",29900016,958,null,129,111,160,124,174]
[null,"1-Month Rental: Accredited Pre-Calibration Certificate DANAK - TMP TSP Dual Sensor",29900137,1157,null,156,135,193,150,210]
[null,"Pressure: Choose from Ambient Temp., 3 PRS points."]
[null,"1-Month Rental: Accredited Pre-Calibration Certificate DANAK - PRS, TSP Pressure Sensor",29900122,1259,null,169,146,210,164,229]
[null,"Relative Humidity: Standard points."]
[null,"1-Month Rental: Accredited Pre-Calibration Certificate DANAK - RH/TMP, TSP RH 5.2 Sensor",29900124,1259,null,169,146,210,164,229]
[]
[null,"TRACKSENSE LYOPRO"]
[null,"TRACKSENSE LYOPRO SYSTEM"]
[null,"All prices are per month"]
[null,"1-Month Rental: TrackSense LyoPro ReaderStation",29311020,6946,null,935,808,1158,902,1263]
[null,"1-Month Rental: TrackSense LyoPro AccessPoint",29311021,5140,null,692,598,857,668,935]
[null,"1-Month Rental: TrackSense LyoPro Logger with 30 cm TC sensor AWG 30 incl. battery",29351250,2643,null,356,307,441,343,481]
[null,"MANDATORY AS FOUND CALIBRATION AFTER RETURN"]
[null,"\"as found\" calibration certificate after return"]
[null,"1-Month Rental: Mandatory Calibration TMP TC Sensor",29900008,1212,null,163,141,202,157,220]
[]
[null,"E-VAL PRO"]
[null,"E-VAL PRO VALIDATION SYSTEM"]
[null,"All prices are per month\nIncludes ValSuite Pro Software license for 2 Computers. The software is validated, 21 CFR part 11 compliant and developed according to GAMP."]
[null,"1-Month Rental: E-Val Pro Plus Module (requires Valsuite 6.5 or later)",29600020,14363,null,1933,1670,2394,1865,2611]
[null,"E-VAL PRO SENSOR ARRAYS"]
[null,"All prices are per month"]
[null,"1-Month Rental: E-Val Pro 12-Channel Array",29600010,1982,null,267,230,330,257,360]
[null,"1-Month Rental: E-Val Pro 4-Channel Array",29600011,706,null,95,82,118,92,128]
[null,"1-Month Rental: E-Val Pro 12-Channel Galvanic Array",29600013,2221,null,299,258,370,288,404]
[null,"1-Month Rental: E-Val Pro 4-Channel Galvanic Array",29600012,1184,null,159,138,197,154,215]
[null,"PROBES AND SENSORS FOR RENT"]
[null,"All prices are per month\nFor Pre-Calibrated Probes, Calibration Points: 0, 121, 135°C"]
[null,"1-Month Rental: STC - Flexible PTFE probe ø3,2 mm x 7 m cable, up to +200°C, w smart USB Connector",29602500,755,null,102,88,126,98,137]
[null,"1-Month Rental: Pre-Cal STC - Flex PTFE probe ø3,2mmx7m cable, up to +200°C, w smart USB Connector",29602501,965,null,130,112,161,125,175]
[null,"1-Month Rental: STC - Flexible PTFE probe ø2,2 mm x 7 m cable, up to +200°C, w smart USB Connector",29602502,767,null,103,89,128,100,139]
[null,"1-Month Rental: Pre-Cal STC - Flex PTFE probe ø2,2mmx7m cable, up to +200°C, w smart USB Connector",29602503,985,null,133,115,164,128,179]
[null,"1-Month Rental: TSP Pressure Sensor including EVP Sensor Interface",29602541,4278,null,576,497,713,556,778]
[null,"1-Month Rental: TSP RH/Temp 5.2 Sensor including EVP Sensor Interface",29602542,3473,null,467,404,579,451,631]
[null,"MANDATORY AS FOUND CALIBRATION AFTER RETURN"]
[null,"Temperature: \"as found\" calibration certificate after return - 3 standard points."]
[null,"1-Month Rental: Mandatory Calibration - TMP Thermocouple",29902150,404,null,54,47,67,52,73]
[null,"Pressure: \"as found\" calibration certificate after return - standard points."]
[null,"1-Month Rental: Mandatory Calibration - PRS Sensor, Std. Points or 1 Custom",29902158,1007,null,136,117,168,131,183]
[null,"Array: \"as found\" calibration certificate after return  - standard points"]
[null,"1-Month Rental: Mandatory Calibration - EVP, 40-Channel, Std Points",29902140,3961,null,533,461,660,514,720]
[null,"Relative Humidity: \"as found\" calibration certificate after return - standard points."]
[null,"1-Month Rental: Mandatory Calibration - RH/TMP, TSP RH 5.2 Sensor",29902159,1007,null,136,117,168,131,183]
[null,"DANAK - ACCREDITED CALIBRATION\nAdditional charge 25%.\nPlease inform customer name for certificate."]
[null,"DANAK TMP - Accredited Calibration Certificate DANAK for Temperature",9000090,0,null,0,0,0,0,0]
[null,"OPTIONAL ACCREDITED PRE-CAL. CERTIFICATE"]
[null,"Please inform full customer name for certificate"]
[null,"1-Month Rental: Accredited Pre-Calibration Certificate DANAK - EVP, 40-Channel",29902240,4949,null,666,575,825,643,900]
[null,"1-Month Rental: Accredited Pre-Calibration Certificate DANAK - PRS, TSP Pressure Sensor",29902258,1259,null,169,146,210,164,229]
[null,"1-Month Rental: Accredited Pre-Calibration Certificate DANAK - RH/TMP, TSP RH 5.2 Sensor",29902259,1253,null,169,146,209,163,228]
[]
[]
[null,"* Some additional items might be available for rental from DACH"]

{"sheet":"Calibration","index":7,"n_rows":141,"n_cols":10,"rows_kept":141,"cut":false,"hidden":false,"merged":[[0,8,1,9],[9,1,9,9],[11,1,11,9],[31,1,31,9],[137,1,137,9],[84,1,84,9],[25,1,25,9],[27,1,27,9],[88,1,88,9],[90,1,90,9],[124,1,124,9],[126,1,126,9],[36,1,36,9],[46,1,46,9],[54,1,54,9],[98,1,98,9],[139,1,139,9],[40,1,40,9],[43,1,43,9],[50,1,50,9],[58,1,58,9],[79,1,79,9],[131,1,131,9],[65,1,65,9],[100,1,100,9],[109,1,109,9],[73,1,73,9],[104,1,104,2],[75,1,75,9],[94,1,94,9]]}
[null,"Ellab Validation Solutions",null,null,null,null,null,null,{"$error":"#VALUE!"}]
[null,"Parts List: Calibration"]
[null,"Validation Pricing Ver. 03 - July 2026"]
[null,"15 July 2026 to 31 December 2026"]
[null,null,null,null,null,"DKK/€","DKK/£","DKK/$","DKK/CHF","DKK/Japan US"]
[null,null,null,null,null,7.43,8.6,6,7.7,5.5]
[null,"Description","Ellab Ordering\nCode","RRP DKK","Discount","RRP €","RRP £","RRP US$","RRP CHF","Japan US$"]
[null,"TRACKSENSE PRO"]
[null,"CALIBRATION OF TS PRO SENSORS INCL. AS FOUND DATA (HISTORIC)"]
[null,"Recommended every year.\n"]
[null,"TEMPERATURE"]
[null,"15 working days\nStandard Calibration Points: 0, 60, 90, 120, 140°C\nLow Temperature Calibration Points:  0, 25, 50, 75, 100°C\nHigh Temperature Calibration Points: 0, 90, 160, 240, 360, 400°C \nThermecouple Sensor: -60, -30, 0, 30, 60°C\nFrigo Logger Calibration Points: -90, -30, 0, 40 and 85°C\nFrigo UX Sky Logger Calibration points: -90, -40, 0, 60, 140°C"]
[null,"CALIBRATION TMP 1 - Re-calibration of single channel sensor",9000005,1947,null,262,226,325,253,354]
[null,"CALIBRATION TMP 2 - Re-calibration of double channel sensor",9000037,2931,null,394,341,489,381,533]
[null,"CALIBRATION TMP 4 - Re-calibration of Quadro channel sensor",9000040,4848,null,652,564,808,630,881]
[null,"CALIB. TC SENSOR - Re-calibration of TC sensor",9000160,3889,null,523,452,648,505,707]
[null,"CAL. COMPACT X - Re-calibration of Compact X logger including -50°C",9000008,2284,null,307,266,381,297,415]
[null,"CAL COMPACT ULTRA X - Re-calibration of Compact Ultra X logger including -80°C",9000009,2499,null,336,291,417,325,454]
[null,"RE-CALIB. FRIGO 15 - Re-calibration of Frigo Logger",9000057,2542,null,342,296,424,330,462]
[null,"Re-calibration of TSP Frigo SKY UX single sensor, DDA Calibration, full spec",9000109,2499,null,336,291,417,325,454]
[null,"TEMPERATURE: EXTRA CHECK POINTS"]
[null,"CALIBRATION -30 C - Additional check point at -30°C, charge per channel",9000059,376,null,51,44,63,49,68]
[null,"CALIBRATION -50 C - Additional check point at -50°C, charge per channel",9000028,376,null,51,44,63,49,68]
[null,"CALIBRATION -80 C. - Additional check point at -80°C, charge per channel",9000029,552,null,74,64,92,72,100]
[null,"CALIBRATION -196 C - Additional check point at -196°C, charge per channel",9000031,611,null,82,71,102,79,111]
[null,"Mandatory start-up fee for other calibration points than already defined as standard points or additional check points  (-30, -50, -80 and -196°C)."]
[null,"Calibration - Custom Setup Fee for Extra Check Points",9000170,1011,null,136,118,169,131,184]
[null,"Extra calibration charge for other calibration points than already defined as standard points or additional check points  (-30, -50, -80 and -196°C).\nFor TSP Single Sensor and Thermocouples use 09000171.\nFor TSP Double Sensor and Frigo, Compact, Compact X and Compact UX Loggers use 09000172"]
[null,"Calibration - Temperature, TSP Single Sensor and TC - Charge for other additional calibration points",9000171,860,null,116,100,143,112,156]
[null,"Calibration - Temperature, TSP - Charge for other additional calibration points",9000172,1117,null,150,130,186,145,203]
[null,"PRESSURE"]
[null,"4 bar - Calibration Points: Pressure: 50, 1000, 3000, 4000 mbar, Temperature: 25, 70, 140°C\n6 bar - Calibration Points: Pressure: 50, 1000, 3500, 6000 mbar, Temperature: 0, 70, 140°C\n8 bar - Calibration Points: Pressure: 50, 1000, 3500, 6000, 8000 mbar, Temperature: 0, 70, 140°C"]
[null,"CALIBRATION PRES - Re-calibration of pressure sensor 15 working days",9000022,3445,null,464,401,574,447,626]
[null,"CALIBRATION PRS/TMP - Re-calibration of combi pressure/1 tmp sensor 15 working days",9000023,5369,null,723,624,895,697,976]
[null,"CAL. BOWIE DICK - Calibration TrackSense Pro Bowie Dick Sensor",9000141,6551,null,882,762,1092,851,1191]
[null,"PRESSURE: EXTRA CHECK POINTS"]
[null,"Mandatory start-up fee for other calibration points than already defined as standard points.\nThe start-up fee applies to each calibration performed at a temperature other than the standard temperature."]
[null,"Calibration - Custom Setup Fee for Extra Check Points",9000170,1011,null,136,118,169,131,184]
[null,"Calibration - Pressure, TSP - Charge for other additional calibration points",9000174,935,null,126,109,156,121,170]
[null,"VACUUM"]
[null,"15 working days"]
[null,"CAL VACUUM - Re-calibration of vacuum/tmp sensor",9000065,6309,null,849,734,1052,819,1147]
[null,"RELATIVE HUMIDITY"]
[null,"Humidity Calibration Points: Relative Humidity: 10, 30, 50, 70, 90%, Temperature: 10, 30, 50, 70, 90°C\n15 working days"]
[null,"CALIBRATION RH - Re-calibration of RH & RH/TMP sensor",9000024,3445,null,464,401,574,447,626]
[null,"RELATIVE HUMIDITY: EXTRA CHECK POINTS"]
[null,"Mandatory start-up fee for other calibration points than already defined as standard points.\nThe start-up fee applies to each calibration performed at a temperature other than the standard temperature."]
[null,"Calibration - Custom Setup Fee for Extra Check Points",9000170,1011,null,136,118,169,131,184]
[null,"Calibration - Relative Humidity, TSP - Charge for other additional calibration points",9000173,1621,null,218,188,270,211,295]
[null,"CONDUCTIVITY"]
[null,"15 working days",null,null,null,0,0,0,0,0]
[null,"CAL CONDUC 0-200 - Re-calibration of conductivity sensor 0-200 µS/cm",9000063,3445,null,464,401,574,447,626]
[null,"CAL CONDUC 200-2000 - Re-calibration of conductivity sensor 200-2000 µS/cm",9000064,3445,null,464,401,574,447,626]
[null,"CONDUCTIVITY: EXTRA CHECK POINTS"]
[null,"Mandatory start-up fee for other calibration points than already defined as standard points."]
[null,"Calibration - Custom Setup Fee for Extra Check Points",9000170,1011,null,136,118,169,131,184]
[null,"Calibration - Conductivity, TSP - Charge for other additional calibration points",9000175,1621,null,218,188,270,211,295]
[null,"CO2"]
[null,"0-10% - Calibration Points: 0, 5, 7.5 and 10%\n0-20% - Calibration Points: 0, 5, 10, 15 and 20%",null,null,null,0,0,0,0,0]
[null,"CAL. CO2 0-10% - Re-calibration of CO2 sensor 0-10%",9000067,2887,null,389,336,481,375,525]
[null,"CAL. CO2 0-20% - Re-calibration of CO2 sensor 0-20%",9000066,4805,null,647,559,801,624,874]
[null,"CHRONOMETRIC"]
[null,"CHRONOMETRIC 23°C - Standard Calibration at 23°C",9000006,599,null,81,70,100,78,109]
[null,"CHRONOMETRIC 70°C - Standard Calibration at 70°C",9000007,773,null,104,90,129,100,141]
[null,"DANAK - ACCREDITED CALIBRATION"]
[null,"Additional charge 25%.\nPlease inform customer name for certificate."]
[null,"DANAK TMP - Accredited Calibration Certificate DANAK for Temperature",9000090,0,null,0,0,0,0,0]
[null,"DANAK RH - Accredited Calibration Certificate DANAK for Relative Humidity",9000091,0,null,0,0,0,0,0]
[null,"DANAK PRS - Accredited Calibration Certificate DANAK for Pressure",9000092,0,null,0,0,0,0,0]
[null,"CERTIFICATES"]
[null,"CERTIFICATE WITH REDUCED REQUIREMENT",9000227,0,null,0,0,0,0,0]
[null,"CALIBRATION CERT. - Calibration certificate, extra copy",9000099,790,null,106,92,132,103,144]
[null,"ADDITIONAL SERVICES"]
[null,"Fast Calibration: Additional charge 50%.\nTemperature and Pressure Calibration Only."]
[null,"CALIBRATION 5 DAYS - Fast re-calibration - 5 working days",9000025,0,null,0,0,0,0,0]
[null,"Minus as found data: less 20% discount\nTS Pro Only."]
[null,"MINUS HISTORIC DATA TSP",9000042,0,null,0,0,0,0,0]
[]
[null,"TRACKSENSE LYOPRO"]
[null,"Thermocouple Sensor:  -60, -30, 0, 30, 60°C"]
[null,"CALIB. TC SENSOR - Re-calibration of TC sensor",9000160,3889,null,523,452,648,505,707]
[]
[null,"TRACKSENSE LAB"]
[null,"CALIBRATION OF SENSORS INCL. AS FOUND DATA (HISTORIC)"]
[null,"Recommended every year.\n15 working days.\nTS Lab Temperature Calibration Points: -30, 0, 40, 70, 100°C\nHumidity / Temperature Calibration Points: 10, 30, 50, 70, 90% RH / 10, 30, 50, 70, 90°C"]
[null,"CALIBRATION TMP 1 - Re-calibration of single channel sensor",9000005,1947,null,262,226,325,253,354]
[null,"CALIBRATION TMP 4 - Re-calibration of Quadro channel sensor",9000040,4848,null,652,564,808,630,881]
[null,"CALIBRATION RH - Re-calibration of RH & RH/TMP sensor",9000024,3445,null,464,401,574,447,626]
[null,"Mandatory start-up fee for other calibration points than already defined as standard points or additional check points  (-30, -50, -80 and -196°C) and Relative Humidity."]
[null,"Calibration - Custom Setup Fee for Extra Check Points",9000170,1011,null,136,118,169,131,184]
[null,"Extra calibration charge for other calibration points than already defined as standard points or additional check points  (-30, -50, -80 and -196°C) and Relative Humidity.\nFor Relative Humidity the start-up fee applies to each calibration performed at a temperature other than the standard temperature."]
[null,"Calibration - Temperature, TSP Single Sensor and TC - Charge for other additional calibration points",9000171,860,null,116,100,143,112,156]
[null,"Calibration - Relative Humidity, TSP - Charge for other additional calibration points",9000173,1621,null,218,188,270,211,295]
[null,"DANAK - ACCREDITED CALIBRATION"]
[null,"Additional charge 25%.\nPlease inform customer name for certificate."]
[null,"DANAK TMP - Accredited Calibration Certificate DANAK for Temperature",9000090,0,null,0,0,0,0,0]
[null,"DANAK RH - Accredited Calibration Certificate DANAK for Relative Humidity",9000091,0,null,0,0,0,0,0]
[null,"ADDITIONAL SERVICES"]
[null,"Fast Calibration: Additional charge 50%.\nTemperature and Pressure Calibration Only."]
[null,"CALIBRATION 5 DAYS - Fast re-calibration - 5 working days",9000025,0,null,0,0,0,0,0]
[null,"Minus as found data: less 20% discount\nTS Pro Only."]
[null,"MINUS HISTORIC DATA TSP",9000042,0,null,0,0,0,0,0]
[]
[null,"STERISENSE"]
[]
[null,"Calibration of SteriSense Unit - max 1000 test cycles",9000140,6551,null,882,762,1092,851,1191]
[]
[null,"E-VAL PRO"]
[null,"CALIBRATION OF ARRAYS AND PROBES"]
[null,"Recommended every year.\n"]
[null,"CALIB. 12 CH EVP - Re-calibration Fee for 12 Channel Array, historic",21610010,3693,null,497,429,616,480,671]
[null,"CALIB. 4 CH EVP - Re-calibration Fee for 4 Channel Array, historic",21610011,2217,null,298,258,370,288,403]
[null,"CAL. EVP PLUG 0-10V - Calibration Fee EVP Plug 0-10V",21610030,1114,null,150,130,186,145,203]
[null,"CAL. EVP PLUG 4-20mA - Calibration Fee EVP Plug 4-20mA",21610031,1114,null,150,130,186,145,203]
[null,"STD. CALIBRATION - Calibration Fee for Probe - 3 points 0, 121, 135°C",21500002,406,null,55,47,68,53,74]
[null,"HIGH CALIBRATION - Calibration Fee for High Temp. Probe - 3 points 200, 300, 400°C",21500006,406,null,55,47,68,53,74]
[null,"HIGH CALIBRATION - Calibration Fee for High Temp. Kapton Probe - 4 points 0, 150, 250, 350°C",21500010,406,null,55,47,68,53,74]
[null,"CALIBRATION PRESSURE - Re-calibration Fee for Digital Pressure Sensor",21500008,6029,null,811,701,1005,783,1096]
[null,"HISTORIC PROBE - Additional historic re-calibration for probe",9000043,406,null,55,47,68,53,74]
[null,"TEMPERATURE: EXTRA CHECK POINTS"]
[null,"CALIB EVP -30°C - Additional check point at -30 °C, charge per channel",9000132,296,null,40,34,49,38,54]
[null,"CALIB EVP -50°C - Additional check point at -50°C, charge per channel",9000128,296,null,40,34,49,38,54]
[null,"CALIB EVP -80°C - Additional check point at -80°C, charge per channel",9000129,296,null,40,34,49,38,54]
[null,"CALIB EVP -196 C - Additional check point at -196°C, charge per channel",9000131,374,null,50,43,62,49,68]
[null,"Mandatory start-up fee for other calibration points than already defined as standard points or additional check points  (-30, -50, -80 and -196°C)."]
[null,"Calibration - Custom Setup Fee for Extra Check Points",9000170,1011,null,136,118,169,131,184]
[null,"An additional calibration charge applies for calibration points other than the defined standard points or additional check points (−30, −50, −80, and −196 °C) within the temperature range of −80 to +400 °C.\nFor calibration of arrays using probes other than type T, a type T calibration is included."]
[null,"Calibration - EVP Probe - Charge for other additional calibration points",9000127,860,null,116,100,143,112,156]
[null,"Calibration - EVP Array, 12 CH - Charge for calibration for other than type T Probes",9000125,7390,null,995,859,1232,960,1344]
[null,"Calibration - EVP Array, 4 CH - Charge for calibration for other than type T Probes",9000126,4435,null,597,516,739,576,806]
[null,"DANAK - ACCREDITED CALIBRATION"]
[null,"Additional charge 25%.\nPlease inform customer name for certificate."]
[null,"DANAK TMP - Accredited Calibration Certificate DANAK for Temperature",9000090,0,null,0,0,0,0,0]
[null,"DANAK PRS - Accredited Calibration Certificate DANAK for Pressure",9000092,0,null,0,0,0,0,0]
[null,"CERTIFICATES"]
[null,"CALIB EVF&P CERT - Calibration certificate, extra copy",9000199,792,null,107,92,132,103,144]
[null,"ADDITIONAL SERVICES"]
[null,"Fast Calibration: Additional charge 50%.\nTemperature and Pressure Calibration Only."]
[null,"CALIBRATION 5 DAYS - Fast re-calibration - 5 working days",9000025,0,null,0,0,0,0,0]
[null,"Minus as found data: less 20% discount\nArrays Only."]
[null,"MINUS HISTORIC DATA ARRAY EVP",21610020,0,null,0,0,0,0,0]

{"sheet":"Service and Documentation","index":8,"n_rows":36,"n_cols":10,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
[null,"Ellab Validation Solutions",null,null,null,null,null,null,{"$error":"#VALUE!"}]
[null,"Parts List: Service and Documentation"]
[null,"Validation Pricing Ver. 03 - July 2026"]
[null,"15 July 2026 to 31 December 2026"]
[null,null,null,null,null,"DKK/€","DKK/£","DKK/$","DKK/CHF","DKK/Japan US"]
[null,null,null,null,null,7.43,8.6,6,7.7,5.5]
[null,"Description","Ellab Ordering\nCode","RRP DKK","Discount","RRP €","RRP £","RRP US$","RRP CHF","Japan US$"]
[null,"SERVICE AGREEMENTS"]
[null,"Service agreement for Calibration of Validation Equipment\n(Details to be found in template)\nOBS! Might not be available in all countries, please consult your VP of Sales"]
[null,"Validation Service Agreement for Calibration - Bronze",20001010,0,null,0,0,0,0,0]
[null,"Validation Service Agreement for Calibration - Silver",20001011,0,null,0,0,0,0,0]
[null,"Validation Service Agreement for Calibration - Gold",20001012,0,null,0,0,0,0,0]
[]
[null,"SERVICE, SUPPORT & TRAINING"]
[null,"REPAIR"]
[null,"REPAIR HOURS - Service hour/examination cost per hour",9000300,1147,null,154,133,191,149,209]
[]
[null,"TRAINING"]
[]
[null,"TRAINING HOUR - Validation/training per hour",10019600,1562,null,210,182,260,203,284]
[null,"TRAINING DAY - Validation/training one day (max. 9 hours)",10019601,12380,null,1666,1440,2063,1608,2251]
[null,"TRAINING WEEK - Validation/training one week (max. 5 days), excl. travel costs",10019602,49473,null,6659,5753,8246,6425,8995]
[null,"SOFTWARE SUPPORT"]
[]
[null,"SOFTWARE SUPPORT - Software support per hour",9000301,1945,null,262,226,324,253,354]
[null,"STD INST. SUPPORT - Standard User Installation Support Package (includes up to 4 hours)",9000303,0,null,0,0,0,0,0]
[null,"SERV. INSTAL. SUP. - Server Installation Support Package (includes up to 8 hours)",9000304,7760,null,1044,902,1293,1008,1411]
[null,"CITRIX INSTAL. SUP. - Citrix Installation Support Package (includes up to 8 hours)",9000305,7760,null,1044,902,1293,1008,1411]
[]
[null,"DOCUMENTATION"]
[]
[null,"VALIDATION REPORT - EVP, Validation of Customer's Equipment according to Ellab's IQ/OQ protocols",21300006,39378,null,5300,4579,6563,5114,7160]
[null,"ValSuite Pro Validation Package - Complete with IQ/OQ tests, test overview, report and statement",21300003,29077,null,3913,3381,4846,3776,5287]
[null,"VALIDATION REPORT - TSP, Validation of Customer's Equipment according to Ellab's IQ/OQ protocols",31182009,39035,null,5254,4539,6506,5069,7097]
[null,"CP / URS Hard Copy",31182050,7314,null,984,850,1219,950,1330]
[null,"CP / URS Electronic Copy",31182051,7314,null,984,850,1219,950,1330]

{"sheet":"Version Control","index":9,"n_rows":8,"n_cols":9,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,7,1,8]]}
[null,null,null,null,null,null,null,{"$error":"#VALUE!"}]
[]
[]
[null,null,null,null,"Exchange Rates"]
[null,"Version","Release Date","Notes","DKK/€","DKK/£","DKK/$","DKK/CHF","DKK/Japan US"]
[null,1,"December 18, 2025","First version in new format",7.43,8.6,6,7.7,5.5]
[null,2,"March 30, 2026","New items added, description updates and editorials"]
[null,3,"July 15, 2026","Price increase, new items added, description updates and editorials"]